{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["表紙","設計内訳書"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":8,"defined_names":189,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"表紙","index":0,"n_rows":24,"n_cols":10,"rows_kept":24,"cut":false,"hidden":false,"merged":[[23,0,42,4],[23,5,25,5],[23,6,25,7],[23,8,25,8],[23,9,25,10],[26,5,42,10],[16,0,19,0],[16,1,19,2],[16,3,19,4],[16,5,18,5],[16,6,18,10],[19,5,22,5],[19,6,22,7],[19,8,22,8],[19,9,22,10],[20,0,22,4],[12,0,15,0],[12,1,13,1],[12,2,13,2],[12,3,13,3],[12,4,13,10],[14,1,15,1],[14,2,15,2],[14,3,15,3],[14,4,15,10],[0,0,3,0],[0,1,3,10],[4,0,7,0],[4,1,7,10],[8,0,11,0],[8,1,11,1],[8,2,11,2],[8,3,11,4],[8,5,11,5]]}
[3,"工事設計書"]
[]
[]
[]
["工事名","令和３年度　青山ホールトイレ改修工事"]
[]
[]
[]
["施工場所",null,"伊賀市","阿保",null,"地内"]
[]
[]
[]
["設計金額"]
[]
[]
[]
["工事期間","契約の日から　　",null,"令和4年1月7日　まで",null,"設計","2021-08-01"]
[]
[]
[null,null,null,null,null,"設計",null,null,"検算"]
["工事概要"]
[]
[]
["青山ホールにおけるトイレ改修工事（和洋改修）\n1階ホールトイレ（男性用トイレ・女性用トイレ）\n1階リハーサル室トイレ（男性用トイレ・女性用トイレ）\n2階トイレ（男性用トイレ・女性用トイレ）",null,null,null,null,"工種","管",null,"コード","09"]

{"sheet":"設計内訳書","index":1,"n_rows":1282,"n_cols":9,"rows_kept":1282,"cut":false,"hidden":false,"merged":[[0,7,1,7],[0,8,1,8],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6]]}
[null,"用途","名　　　　称","摘　　　　　　　要","数　　量","単位","単　　価","金　　額","備　　　考"]
[]
[]
[1,null,"令和3年度　青山ホールトイレ改修工事",null," "]
[]
[2]
[]
[3,"A","直接工事費",null,1,"式"]
[]
[4,"B","共通仮設費","共通仮設費率",1,"式"]
[]
[5]
[]
[6]
[]
[7,null,"純工事費"]
[]
[8]
[]
[9,"C","現場管理費","現場管理費率",1,"式"]
[]
[10]
[]
[11,null,"工事原価"]
[]
[12]
[]
[13,"D","一般管理費",null,1,"式"]
[]
[14]
[]
[15,null,"工事価格"]
[]
[16]
[]
[17,null,"消費税及び地方消費税額",null,1,"式"]
[]
[18]
[]
[19,null,"設計金額"]
[]
[20]
[]
[1,null,null,null," "]
[]
[2,"A","直接工事費"]
[]
[3,1,"改修建築工事","発生材処理費を含む",1,"式"]
[]
[4,2,"改修電気設備工事",null,1,"式"]
[]
[5,3,"改修機械設備工事",null,1,"式"]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"A　の計"]
[]
[1,null,null,null," "]
[]
[2,1,"改修建築工事"]
[]
[3,"a","1階ホール男性用トイレ",null,1,"式"]
[]
[4,"b","1階ホール女性用トイレ",null,1,"式"]
[]
[5,"c","1階リハーサル室男性用トイレ",null,1,"式"]
[]
[6,"d","1階リハーサル室女性用トイレ",null,1,"式"]
[]
[7,"e","2階男性用トイレ",null,1,"式"]
[]
[8,"f","2階女性用トイレ",null,1,"式"]
[]
[9,"ｇ","廃材運搬費",null,1,"式"]
[]
[10,"ｈ","廃材処分費",null,1,"式"]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"1　の計"]
[]
[1,null,null,null," "]
[]
[2,"a","1階ホール男性用トイレ"]
[]
[3,null,"床養生","養生シート及びベニヤ板　共用部を含む",73.2,"㎡"]
[]
[4,null,"整理清掃後片付け",null,18.600000000000001,"㎡"]
[]
[5,null,"トイレブース撤去","撤去跡補修とも",13.8,"㎡"]
[null,null,null,null,null,null,"",""]
[6,null,"衛生器具撤去",null,1,"式","","（改修機械設備工事）"]
[]
[7]
[]
[8,null,"カッター入れ","コンクリート面+モルタル面",9.8000000000000007,"ｍ"]
[]
[9,null,"床タイル撤去","下地モルタルとも",1.8,"㎡"]
[]
[10,null,"土間コンクリート撤去","コンクリートブレーカ",0.2,"㎥"]
[]
[11,null,"掘削","人力",0.7,"㎥"]
[]
[12,null,"埋戻し","人力　クッション砂",0.6,"㎥"]
[]
[13,null,"発生土積込","人力",0.7,"㎥"]
[]
[14,null,"砂利事業","再生クラッシャラン",0.2,"㎥"]
[]
[15,null,"床下防湿層敷き","ポリエチレンフィルム　厚0.15mm",1.8,"㎡"]
[]
[16,null,"コンクリート補修","Fc21N　S18",0.2,"㎥"]
[]
[17,null,"モルタル塗木ごて押え","床タイル下",1.8,"㎡"]
[]
[18,null,"床タイル補修","磁器質　100角",1.8,"㎡"]
[]
[19]
[]
[20]
[]
[1,null,null,null," "]
[null,null,null,"メラミン樹脂化粧板　厚40mm"]
[2,null,"TS-4","金物類、運搬費、取付費を含む",1,"個所"]
[]
[3]
[]
[4,null,"シーリング","MS-2　TS-2、洗面カウンター取合い",1.3,"ｍ"]
[]
[5]
[]
[6,null,"天井点検口","450*450　アルミ枠",3,"個所"]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"a　の計"]
[]
[1]
[]
[2,"b","1階ホール女性用トイレ"]
[]
[3,null,"養生費","養生シート及びベニヤ板",31.8,"㎡"]
[]
[4,null,"整理清掃後片付け",null,17.3,"㎡"]
[]
[5,null,"トイレブース撤去","撤去跡補修とも",14,"㎡"]
[null,null,null,null,null,null,"",""]
[6,null,"衛生器具撤去",null,1,"式","","（改修機械設備工事）"]
[]
[7]
[]
[8,null,"カッター入れ","コンクリート面+モルタル面",14.1,"ｍ"]
[]
[9,null,"床タイル撤去","下地モルタルとも",3.1,"㎡"]
[]
[10,null,"土間コンクリート撤去","コンクリートブレーカ",0.4,"㎥"]
[]
[11,null,"掘削","人力",1.2,"㎥"]
[]
[12,null,"埋戻し","人力　クッション砂",0.9,"㎥"]
[]
[13,null,"発生土積込","人力",1.2,"㎡"]
[]
[14,null,"砂利事業","再生クラッシャラン",0.3,"㎡"]
[]
[15,null,"床下防湿層敷き","ポリエチレンフィルム　厚0.15mm",3.1,"㎡"]
[]
[16,null,"コンクリート補修","Fc21N　S18",0.4,"㎥"]
[]
[17,null,"モルタル塗木ごて押え","床タイル下",3.1,"㎡"]
[]
[18,null,"床タイル補修","磁器質　100角",3.1,"㎡"]
[]
[19]
[]
[20]
[]
[1]
[null,null,null,"高圧メラミン樹脂化粧板　厚40mm"]
[2,null,"TS-3","金物類、運搬費、取付費を含む",1,"個所"]
[]
[3]
[]
[4,null,"天井点検口","450*450　アルミ枠",3,"個所"]
[]
[5]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15,null,null,null," "]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"ｂ　の計"]
[]
[1]
[]
[2,"c","1階リハーサル室男性用トイレ"]
[]
[3,null,"養生費","養生シート及びベニヤ板　共用部を含む",25.3,"㎡"]
[]
[4,null,"整理清掃後片付け",null,8.4,"㎡"]
[]
[5,null,"トイレブース撤去",null,6.8,"㎡"]
[null,null,null,null,null,null,"",""]
[6,null,"衛生器具撤去",null,1,"式","","（改修機械設備工事）"]
[]
[7]
[]
[8,null,"カッター入れ","コンクリート面+モルタル面",4,"ｍ"]
[]
[9,null,"床タイル撤去","下地モルタルとも",0.8,"㎡"]
[]
[10,null,"土間コンクリート撤去","コンクリートブレーカ",0.1,"㎥"]
[]
[11,null,"掘削","人力",0.3,"㎥"]
[]
[12,null,"埋戻し","人力　クッション砂",0.3,"㎥"]
[]
[13,null,"発生土積込","人力",0.3,"㎡"]
[]
[14,null,"砂利事業","再生クラッシャラン",0.1,"㎡"]
[]
[15,null,"床下防湿層敷き","ポリエチレンフィルム　厚0.15mm",0.8,"㎡"]
[]
[16,null,"コンクリート補修","Fc21N　S18",0.1,"㎥"]
[]
[17,null,"モルタル塗木ごて押え","床タイル下",0.8,"㎡"]
[]
[18,null,"床タイル補修","磁器質　100角",0.8,"㎡"]
[]
[19]
[]
[20]
[]
[1]
[null,null,null,"高圧メラミン樹脂化粧板　厚40mm"]
[2,null,"TS-2","金物類、運搬費、取付費を含む",1,"個所"]
[]
[3]
[]
[4,null,"シーリング","MS-2　TS-2、洗面カウンター取合い",0.7,"ｍ"]
[]
[5]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12,null,null,null," "]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"ｃ　の計"]
[]
[1]
[]
[2,"d","1階リハーサル室女性用トイレ"]
[]
[3,null,"養生費","養生シート及びベニヤ板",10.199999999999999,"㎡"]
[]
[4,null,"整理清掃後片付け",null,8.6999999999999993,"㎡"]
[]
[5,null,"トイレブース撤去","撤去跡補修とも",15.8,"㎡"]
[null,null,null,null,null,null,"",""]
[6,null,"衛生器具撤去",null,1,"式","","（改修機械設備工事）"]
[]
[7]
[]
[8,null,"カッター入れ","コンクリート面+モルタル面",3,"ｍ"]
[]
[9,null,"床タイル撤去","下地モルタルとも",0.8,"㎡"]
[]
[10,null,"土間コンクリート撤去","コンクリートブレーカ",0.1,"㎥"]
[]
[11,null,"掘削","人力",0.3,"㎥"]
[]
[12,null,"埋戻し","人力　クッション砂",0.3,"㎥"]
[]
[13,null,"発生土積込","人力",0.3,"㎡"]
[]
[14,null,"砂利事業","再生クラッシャラン",0.1,"㎡"]
[]
[15,null,"床下防湿層敷き","ポリエチレンフィルム　厚0.15mm",0.8,"㎡"]
[]
[16,null,"コンクリート補修","Fc21N　S18",0.1,"㎥"]
[]
[17,null,"モルタル塗木ごて押え","床タイル下",0.8,"㎡"]
[]
[18,null,"床タイル補修","磁器質　100角",0.8,"㎡"]
[]
[19]
[]
[20]
[]
[1]
[null,null,null,"高圧メラミン樹脂化粧板　厚40mm"]
[2,null,"TS-1","金物類、運搬費、取付費を含む",1,"個所"]
[]
[3,null,null,null," "]
[]
[4,null,"天井点検口","450*450　アルミ枠",3,"個所"]
[]
[5]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"d　の計"]
[]
[1]
[]
[2,"e","2階男性用トイレ"]
[]
[3,null,"養生費","養生シート及びベニヤ板　1階楽屋を含む",19.100000000000001,"㎡"]
[]
[4,null,"整理清掃後片付け",null,4.4000000000000004,"㎡"]
[]
[5,null,"トイレブース撤去","撤去跡補修とも",5.8,"㎡"]
[null,null,null,null,null,null,"",""]
[6,null,"衛生器具撤去",null,1,"式","","（改修機械設備工事）"]
[]
[7]
[]
[8,null,"カッター入れ","コンクリート面+モルタル面",3.6,"ｍ"]
[]
[9,null,"床タイル撤去","下地モルタルとも",0.8,"㎡"]
[]
[10,null,"土間コンクリート撤去","コンクリートブレーカ",0.1,"㎥"]
[]
[null,null,"設備壁撤去","コンクリートブロック積み",0.1,"㎥"]
[]
[11,null,"型わく",null,0.8,"㎥"]
[]
[12,null,"屋内アスファルト防水","E-1　密着工法　平部",0.8,"㎥"]
[]
[13,null,"コンクリート補修","Fc21N　S18",0.1,"㎥"]
[]
[14,null,"モルタル塗木ごて押え","床タイル下",0.8,"㎡"]
[]
[15,null,"床タイル補修","磁器質100角",0.8,"㎡"]
[]
[16,null,"モルタル補修","防水モルタル　トイレブース撤去跡小口",1.2,"ｍ"]
[]
[17]
[null,null,null,"高圧メラミン樹脂化粧板　厚40mm"]
[18,null,"TS-7","金物類、運搬費、取付費を含む",1,"個所"]
[]
[20]
[]
[1]
[]
[2,null,"シーリング","MS-2　TS-7、洗面カウンター取合い",0.7,"ｍ"]
[]
[3,null,null,"MS-2　TS-7、設備壁取合い",1.3,"ｍ"]
[]
[4]
[]
[5,null,"内部足場","脚立足場　並列",8.4,"㎡"]
[]
[6,null,"天井ボード撤去","（1階）　化粧石膏ボード",8.4,"㎡"]
[]
[7,null,"天井不燃化粧せっこうボード張り","（1階）　厚9.5　不燃　突付け",8.4,"㎡"]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"e　の計"]
[]
[1]
[]
[2,"f","2階女性用トイレ"]
[]
[3,null,"養生費","養生シート及びベニヤ板　共用部、1階シャワー室を含む",44.3,"㎡"]
[]
[4,null,"整理清掃後片付け",null,8.1999999999999993,"㎡"]
[]
[5,null,"トイレブース撤去","撤去跡補修とも",11.3,"㎡"]
[null,null,null,null,null,null,"",""]
[6,null,"衛生器具撤去",null,1,"式","","（改修機械設備工事）"]
[]
[7]
[]
[8,null,"カッター入れ","コンクリート面+モルタル面",3.2,"ｍ"]
[]
[9,null,"床タイル撤去","下地モルタルとも",0.6,"㎡"]
[]
[10,null,"土間コンクリート撤去","コンクリートブレーカ",0.1,"㎥"]
[]
[11,null,"型わく",null,0.6,"㎥"]
[]
[12,null,"屋内アスファルト防水","E-1　密着工法　平部",0.6,"㎥"]
[]
[13,null,"コンクリート補修","Fc21N　S18",0.1,"㎥"]
[]
[14,null,"モルタル塗木ごて押え","床タイル下",0.6,"㎡"]
[]
[15,null,"床タイル補修","磁器質　100角",0.6,"㎡"]
[]
[16]
[null,null,null,"高圧メラミン樹脂化粧板　厚40mm"]
[17,null,"TS-5","金物類、運搬費、取付費を含む",1,"個所"]
[null,null,null,"高圧メラミン樹脂化粧板　厚40mm"]
[18,null,"TS-6","金物類、運搬費、取付費を含む",1,"個所"]
[]
[19]
[]
[20]
[]
[1]
[]
[2,null,"シーリング","MS-2　TS-5、洗面カウンター取合い",0.7,"ｍ"]
[]
[3,null,null,"MS-2　TS-5、設備壁取合い",2.7,"ｍ"]
[]
[4,null,null,null," "]
[]
[5,null,"天井点検口","450*450　アルミ枠",1,"個所"]
[]
[6]
[]
[7,null,"内部足場","脚立足場　並列",4.0999999999999996,"㎡"]
[]
[8,null,"天井ボード撤去","（1階）　けい酸カルシウム板（アスベスト含有）　廻り縁とも",2,"㎡"]
[]
[9,null,null,"（1階）　浴室天井材　捨て貼り　廻り縁とも　",2,"㎡"]
[]
[10,null,"天井けい酸カルシウム板張り","（1階）　厚6.0　不燃　目透し",2,"㎡"]
[]
[11,null,null,"（1階）　浴室天井材　硬質塩ビ製　廻り縁とも",2,"㎡"]
[]
[null,null,"天井耐水合板張り","（1階）　浴室天井材下地",2,"㎡"]
[]
[12,null,"廻り縁","塩ビ製",5.7,"ｍ"]
[]
[13,null,"EP塗り","ケイ酸カルシウム板面　素地ごしらえB種とも",2,"㎡"]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"f　の計"]
[]
[1]
[]
[2,"g","廃材運搬費"]
[]
[3,null,"コンクリートがら",null,1,"㎥"]
[]
[4,null,"がれき類","衛生器具、タイル",5.7,"㎥"]
[]
[5,null,"廃プラスチック類","衛生器具、管類",0.1,"㎥"]
[]
[6,null,"木くず",null,2.7,"㎥"]
[]
[7,null,"金属くず",null,0.1,"㎥"]
[]
[8,null,"ボード類",null,0.1,"㎥"]
[]
[9,null,"発生土",null,2.5,"㎥"]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"g　の計"]
[]
[1]
[]
[2,"ｈ","廃材処分費"]
[]
[3,null,"コンクリートがら",null,1.8,"t"]
[]
[4,null,"がれき類","衛生器具、タイル",5.7,"t"]
[]
[5,null,"廃プラスチック類","衛生器具、管類",0.04,"t"]
[]
[6,null,"木くず",null,1.6,"t"]
[]
[7,null,"金属くず",null,0.1,"t"]
[]
[8,null,"ボード類",null,0.02,"t"]
[]
[9,null,"アスベスト含有建材","非飛散性",0.01,"t"]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"ｈ　の計"]
[]
[1,null,null,null," "]
[]
[2,2,"改修電気設備工事"]
[]
[3,"a","1階ホールトイレ",null,1,"式"]
[]
[4,"b","1階リハーサル室トイレ",null,1,"式"]
[]
[5,"c","2階トイレ",null,1,"式"]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"2　の計"]
[]
[1,null,null,null," "]
[]
[2,"a","1階ホールトイレ"]
[]
[3,null,"ケーブル","VVF2.0mm-3C　ころがし配線",74.7,"ｍ"]
[]
[4,null,"結線","１L-2予備回路",1,"式"]
[]
[5,null,"ボックス類",null,1,"式"]
[]
[6,null,"コンセント","2P15A×2　ET付　（露出ボックス，1種金属製線びA型）",7,"個"]
[]
[7]
[]
[8,null,"2種金属製線ぴ","A型",17.5,"ｍ"]
[]
[9,null,"コンセント用ボックス",null,7,"個"]
[]
[10,null,"機械はつり",null,1,"個所"]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"a　の計"]
[]
[1,null,null,null," "]
[]
[2,"b","1階リハーサル室トイレ"]
[]
[3,null,"ケーブル","VVF2.0mm-3C　ころがし配線",37.299999999999997,"ｍ"]
[]
[4,null,"結線","１L-2予備回路",1,"式"]
[]
[5,null,"ボックス類",null,1,"式"]
[]
[6,null,"コンセント","2P15A×2　ET付　（露出ボックス，1種金属製線びA型）",2,"個"]
[]
[7]
[]
[8,null,"2種金属製線ぴ","A型",5,"ｍ"]
[]
[9,null,"コンセント用ボックス",null,2,"個"]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"b　の計"]
[]
[1,null,null,null," "]
[]
[2,"c","2階トイレ"]
[]
[3,null,"ケーブル","VVF2.0mm-3C　ころがし配線",22.6,"ｍ"]
[]
[4,null,"結線","１L-2予備回路",1,"式"]
[]
[5,null,"ボックス類",null,1,"式"]
[]
[6,null,"コンセント","2P15A×2　ET付　（露出ボックス，1種金属製線びA型）",2,"個"]
[]
[7]
[]
[8,null,"2種金属製線ぴ","A型",5,"ｍ"]
[]
[9,null,"コンセント用ボックス",null,2,"個"]
[]
[10,null,"スポット型感知器取外し復旧","定温式　防水型　1階シャワー室",1,"個"]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"c　の計"]
[]
[1,null,null,null," "]
[]
[2,"3","改修機械設備工事"]
[]
[3,"a","1階ホール男性用トイレ",null,1,"式"]
[]
[4,"b","1階ホール女性用トイレ",null,1,"式"]
[]
[5,"c","1階リハーサル室男性用トイレ",null,1,"式"]
[]
[6,"d","1階リハーサル室女性用トイレ",null,1,"式"]
[]
[7,"e","2階男性用トイレ",null,1,"式"]
[]
[8,"f","2階女性用トイレ",null,1,"式"]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"3　の計"]
[]
[1,null,null,null," "]
[]
[2,"a","1階ホール男性用トイレ"]
[]
[3,null,"洋風便器","BC-K21H，DV-K213HM，CF-200S",3,"組"]
[]
[4,null,"棚付2連紙巻器","CF-63HS",3,"組"]
[]
[5,null,"L型手すり","KF-920AE70D12J",3,"組"]
[]
[6,null,"給水管","HIVP20",2.2000000000000002,"ｍ"]
[]
[7,null,"排水管","VP75",2.1,"ｍ"]
[]
[8,null,"配管分岐","25A（給水管）",1,"個所"]
[]
[9,null,null,"32A（給水管）",1,"個所"]
[]
[10,null,null,"40A（給水管）",1,"個所"]
[]
[11,null,null,"100A（排水管）",1,"個所"]
[]
[12,null,"配管切断","32A（給水管）",1,"個所"]
[]
[13,null,null,"40A(給水管）",1,"個所"]
[]
[14,null,null,"75A（排水管）",3,"個所"]
[]
[15]
[]
[16,null,"衛生器具撤去","腰掛便器",1,"組"]
[]
[17,null,null,"和風便器（フラッシュ弁式）",2,"組"]
[]
[18,null,null,"紙巻器",3,"組"]
[]
[19,null,null,"I型手摺　L-300",2,"組"]
[]
[20]
[]
[1]
[]
[2,null,"衛生器具撤去","I型手摺　L-500",2,"組"]
[]
[3,null,"既設管撤去","給水管　HIVP20",2.6,"ｍ"]
[]
[4,null,null,"排水管　VP75",2.5,"ｍ"]
[]
[5]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"a　の計"]
[]
[1,null,null,null," "]
[]
[2,"b","1階ホール女性用トイレ"]
[]
[3,null,"洋風便器","BC-K21H，DV-K213HM，CF-200S",4,"組"]
[]
[4,null,"棚付2連紙巻器","CF-63HS",4,"組"]
[]
[5,null,"L型手すり","KF-920AE70D12J",4,"組"]
[]
[6,null,"給水管","HIVP20",3.3,"ｍ"]
[]
[7,null,"排水管","VP75",3.6,"ｍ"]
[]
[8,null,"配管分岐","32A（給水管）",1,"個所"]
[]
[9,null,null,"40A（給水管）",1,"個所"]
[]
[10,null,null,"75A（排水管）",4,"個所"]
[]
[11,null,"配管切断","20A（給水管）",1,"個所"]
[]
[12,null,null,"25A（給水管）",1,"個所"]
[]
[13,null,null,"32A（給水管）",1,"個所"]
[]
[14,null,null,"40A（給水管）",1,"個所"]
[]
[15,null,null,"75A（排水管）",4,"個所"]
[]
[16]
[]
[17,null,"衛生器具撤去","和風便器（フラッシュ弁式）",3,"組"]
[]
[18,null,null,"和風便器（隅付ロータンク式）",1,"組"]
[]
[19,null,null,"紙巻器",4,"組"]
[]
[20]
[]
[1]
[]
[2,null,"衛生器具撤去","棚",4,"組"]
[]
[3,null,null,"I型手摺　L-300",4,"組"]
[]
[4,null,"既設管撤去","給水管　HIVP20",2.7,"ｍ"]
[]
[5,null,null,"排水管　VP75",3.4,"ｍ"]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"b　の計"]
[]
[1,null,null,null," "]
[]
[2,"c","1階リハーサル室男性用トイレ"]
[]
[3,null,"洋風便器","BC-K21H，DV-K213HM，CF-200S",1,"組"]
[]
[4,null,"棚付2連紙巻器","CF-63HS",1,"組"]
[]
[5,null,"L型手すり","KF-920AE70D12J",1,"組"]
[]
[6,null,"給水管","HIVP20",1.1000000000000001,"ｍ"]
[]
[7,null,"排水管","VP75",1.2,"ｍ"]
[]
[8,null,"配管切断","25A（給水管）",1,"個所"]
[]
[9,null,null,"75A（排水管）",1,"個所"]
[]
[10]
[]
[11,null,"衛生器具撤去","和風便器（フラッシュ弁式）",1,"組"]
[]
[12,null,null,"紙巻器",1,"組"]
[]
[13,null,null,"棚",1,"組"]
[]
[14,null,"既設給水管撤去","HIVP20",0.6,"ｍ"]
[]
[15,null,"既設排水管撤去","VP75",0.5,"ｍ"]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"c　の計"]
[]
[1,null,null,null," "]
[]
[2,"d","1階リハーサル室女性用トイレ"]
[]
[3,null,"洋風便器","BC-K21H，DV-K213HM，CF-200S",1,"組"]
[]
[4,null,"棚付2連紙巻器","CF-63HS",1,"組"]
[]
[5,null,"L型手すり","KF-920AE70D12J",1,"組"]
[]
[6,null,"給水管","HIVP20",0.7,"ｍ"]
[]
[7,null,"排水管","VP75",0.7,"ｍ"]
[]
[8,null,"配管切断","20A（給水管）",1,"個所"]
[]
[9,null,null,"75A（排水管）",1,"個所"]
[]
[10]
[]
[11,null,"衛生器具撤去","和風便器（フラッシュ弁式）",1,"組"]
[]
[12,null,null,"紙巻器",1,"組"]
[]
[13,null,null,"棚",1,"組"]
[]
[14,null,"既設管撤去","給水管　HIVP20",0.6,"ｍ"]
[]
[15,null,null,"排水管　VP75",0.8,"ｍ"]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"d　の計"]
[]
[1,null,null,null," "]
[]
[2,"e","2階男性用トイレ"]
[]
[3,null,"洋風便器","BC-K21H，DV-K213HM，CF-200S",1,"組"]
[]
[4,null,"棚付2連紙巻器","CF-63HS",1,"組"]
[]
[5,null,"L型手すり","KF-920AE70D12J",1,"組"]
[]
[6,null,"給水管","HIVP20",0.7,"ｍ"]
[]
[7,null,"排水管","VP75",1.1000000000000001,"ｍ"]
[]
[8,null,"保温工事","呼び径20mm",0.7,"ｍ"]
[]
[9,null,null,"呼び径75mm",1.1000000000000001,"ｍ"]
[]
[10,null,"配管分岐","75A（排水管）",1,"個所"]
[]
[11,null,"配管切断","25A（給水管）",1,"個所"]
[]
[12,null,null,"75A（排水管）",1,"個所"]
[]
[13]
[]
[14,null,"衛生器具撤去","和風便器（フラッシュ弁式）",1,"組"]
[]
[15,null,null,"紙巻器",1,"組"]
[]
[16,null,null,"棚",1,"組"]
[]
[17,null,"既設管撤去","給水管　HIVP20",0.5,"ｍ"]
[]
[18,null,null,"排水管　VP75",1,"ｍ"]
[]
[19,null,"保温材撤去","呼び径20mm",0.5,"ｍ"]
[]
[20]
[]
[1,null,null,null," "]
[]
[2,null,"保温材撤去","呼び径75mm",1,"ｍ"]
[]
[3]
[]
[4]
[]
[5]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"e　の計"]
[]
[1,null,null,null," "]
[]
[2,"f","2階女性用トイレ"]
[]
[3,null,"洋風便器","BC-K21H，DV-K213HM，CF-200S",1,"組"]
[]
[4,null,"棚付2連紙巻器","CF-63HS",1,"組"]
[]
[5,null,"L型手すり","KF-920AE70D12J",1,"組"]
[]
[6,null,"給水管","HIVP20",0.6,"ｍ"]
[]
[7,null,"排水管","VP75",0.8,"ｍ"]
[]
[8,null,"保温工事","呼び径20mm",0.6,"ｍ"]
[]
[9,null,null,"呼び径75mm",0.8,"ｍ"]
[]
[10,null,"配管切断","25A（給水管）",1,"個所"]
[]
[11,null,null,"75A（排水管）",1,"個所"]
[]
[12]
[]
[13,null,"衛生器具撤去","和風便器（フラッシュ弁式）",1,"組"]
[]
[14,null,null,"紙巻器",2,"組"]
[]
[15,null,null,"棚",2,"組"]
[]
[16,null,"既設管撤去","給水管　HIVP20",1.3,"ｍ"]
[]
[17,null,null,"排水管　VP75",0.7,"ｍ"]
[]
[18,null,"保温材撤去","呼び径20mm",1.3,"ｍ"]
[]
[19,null,null,"呼び径75mm",0.7,"ｍ"]
[]
[20]
[]
[1,null,null,null," "]
[]
[2,null,"換気扇取外し復旧","天井埋込形　1階シャワー室",1,"個"]
[]
[3]
[]
[4]
[]
[5]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"f　の計"]