{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["表紙","設計内訳書"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":8,"defined_names":189,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"表紙","index":0,"n_rows":24,"n_cols":10,"rows_kept":24,"cut":false,"hidden":false,"merged":[[0,0,3,0],[0,1,3,10],[4,0,7,0],[4,1,7,10],[8,0,11,0],[8,1,11,1],[8,2,11,2],[8,3,11,4],[8,5,11,5],[12,0,15,0],[12,1,13,1],[12,2,13,2],[12,3,13,3],[12,4,13,10],[14,1,15,1],[14,2,15,2],[14,3,15,3],[14,4,15,10],[16,0,19,0],[16,1,19,2],[16,3,19,4],[16,5,18,5],[16,6,18,10],[19,5,22,5],[19,6,22,7],[19,8,22,8],[19,9,22,10],[20,0,22,4],[23,0,42,4],[23,5,25,5],[23,6,25,7],[23,8,25,8],[23,9,25,10],[26,5,42,10]]}
[3,"工事設計書"]
[]
[]
[]
["工事名","令和３年度　ゆめぽりすセンター空気調和設備更新工事"]
[]
[]
[]
["施工場所",null,"伊賀市","ゆめが丘",null,"地内"]
[]
[]
[]
["工事費"]
[]
[]
[]
["工事期間","契約の日から　　",null,"令和4年3月16日　まで",null,"設計","2021-10-01"]
[]
[]
[null,null,null,null,null,"設計",null,null,"検算"]
["工事概要"]
[]
[]
["ゆめぽりすセンターにおける空気調和設備の更新\n既設屋外吸収式冷温水発生機及び屋内ファンコイルユニットを撤去、ガスヒートポンプエアコンへ更新\n\n（撤去）吸収式冷温水発生機・密閉型膨張タンク・加圧給水ポンプユニット・防食サイレンサー・ファンコイルユニット（天井カセット形、天井埋込形、床置き隠ぺい形）計３９台・配管一式　※ファンコイルユニットの一部及び天井内配管は存置とする\n\n（更新）ガスヒ－トポンプエアコン屋外機４台（４系統）・屋内機（壁掛け形、天井カセット４方向、天井カセット２方向、天井埋込ダクト形、床置ローボーイ形）計４２台・集中管理リモコンスイッチ・冷媒ガス漏れ感知器\n\n改修機械設備工事に伴う改修建築工事及び改修電気設備工事を含む",null,null,null,null,"工種","管",null,"コード","09"]

{"sheet":"設計内訳書","index":1,"n_rows":1042,"n_cols":9,"rows_kept":1042,"cut":false,"hidden":false,"merged":[[0,7,1,7],[0,8,1,8],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6]]}
[null,"用途","名　　　　称","摘　　　　　　　要","数　　量","単位","単　　価","金　　額","備　　　考"]
[]
[]
[1,null,{"$f":"表紙!B5","v":"令和３年度　ゆめぽりすセンター空気調和設備更新工事"},null," "]
[]
[2]
[]
[3,"A","直接工事費",null,1,"式"]
[]
[4,"B","共通仮設費","共通仮設費率",1,"式"]
[]
[5,null,null,"積上共通仮設費",1,"式"]
[]
[6]
[]
[7,null,"純工事費"]
[]
[8]
[]
[9,"C","現場管理費","現場管理費率",1,"式"]
[]
[10]
[]
[11,null,"工事原価"]
[]
[12]
[]
[13,"D","一般管理費",null,1,"式"]
[]
[14]
[]
[15,null,"工事価格"]
[]
[16]
[]
[17,null,"消費税及び地方消費税額",null,1,"式"]
[]
[18]
[]
[19,null,"工事費"]
[]
[20]
[]
[1,null,null,null," "]
[]
[2,"A","直接工事費"]
[]
[3,"Ⅰ","改修建築工事","発生材処理費を含む",1,"式"]
[]
[4,"Ⅱ","改修電気設備工事",null,1,"式"]
[]
[5,"Ⅲ","改修機械設備工事",null,1,"式"]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"A　の計"]
[]
[1,null,null,null," "]
[]
[2,"Ⅰ","改修建築工事"]
[]
[3,1,"直接仮設工事",null,1,"式"]
[]
[4,2,"鉄筋工事",null,1,"式"]
[]
[5,3,"コンクリート・型枠工事",null,1,"式"]
[]
[6,4,"内装工事",null,1,"式"]
[]
[7,5,"解体工事",null,1,"式"]
[]
[8,6,"発生材積込運搬費",null,1,"式"]
[]
[9,7,"発生材処分費",null,1,"式"]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"1　の計"]
[]
[1,null,null,null," "]
[]
[2,1,{"$f":"C88","v":"直接仮設工事"}]
[]
[3]
[]
[4,null,"内部足場","脚立足場 並列 H=1.8m 2ヶ月",333,"㎡"]
[]
[5]
[]
[6,null,"養生",null,418,"㎡"]
[]
[7,null,"清掃・片付け","施工中",418,"㎡"]
[]
[8,null,"竣工時クリーニング",null,418,"㎡"]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"1　の計"]
[]
[1,null,null,null," "]
[]
[2,2,"鉄筋工事"]
[]
[3,null,"異形鉄筋","SD295A D10",16.7,"kg"]
[]
[4,null,"鉄筋加工組立費",null,16.7,"kg"]
[]
[5]
[]
[6,null,"鉄筋運搬費","16.7kg",1,"式"]
[]
[7]
[null,null,null,"横向き"]
[8,null,"差し筋アンカー","D10",11,"本"]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"2　の計"]
[]
[1]
[]
[2,3,"コンクリート・型枠工事"]
[]
[3,null,"砕石","再生土間下",0.4,"㎥"]
[]
[4,null,"土間コンクリート","Fc21N S18 t=120",0.5,"㎥"]
[]
[5,null,"同上打設手間",null,0.5,"㎥"]
[]
[6]
[]
[7,null,"普通型枠","細幅物（300mm以下）",5.3,"ｍ"]
[]
[8,null,"同上　運搬費",null,5.3,"ｍ"]
[]
[9]
[]
[10,null,"コンクリート直押え",null,2.4,"㎡"]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"3　の計"]
[]
[1]
[]
[2,4,"内装工事"]
[]
[3,null,"天井点検口","アルミ製450角　LGS開口補強含む",50,"ヶ所"]
[]
[4]
[null,null,null,"1階エントランス・2階大会議室"]
[5,null,"天井　岩綿吸音板貼り","t=9（PBt=9.5下貼り共）",7.7,"㎡"]
[null,null,null,"1階事務室・会議室・2階西会議室"]
[6,null,"天井　化粧石膏ボード貼り","t=9.5",4.2,"㎡"]
[]
[7]
[null,null,null,"憩いの広場（右、左）　2,000*D300"]
[8,null,"天井　線状吹き出し口閉塞","PBt=9.5　下地処理　不燃クロス貼り　",2,"ヶ所"]
[null,null,null,"憩いの広場（右、左）　1,250*D450"]
[9,null,"天井　線状吹き出し口閉塞","PBt=9.5　下地処理　不燃クロス貼り　",2,"ヶ所"]
[null,null,null,"憩いの広場（中央）　750*150"]
[10,null,"壁　吹き出し口閉塞","PBt=12.5　下地処理　ジュラククロス貼り　",2,"ヶ所"]
[null,null,null,"憩いの広場（中央）　750*250"]
[11,null,"壁　吹き出し口閉塞","PBt=12.5　下地処理　ジュラククロス貼り　",2,"ヶ所"]
[]
[12]
[]
[13]
[]
[14]
[]
[15,null,null,null," "]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"4　の計"]
[]
[1]
[]
[2,5,"解体工事"]
[]
[3,"（外部）","床カッター切り","土間コンクリート",6,"ｍ"]
[]
[4,null,"土間コンクリート撤去","ハンドブレーカ主体",0.1,"㎥"]
[]
[5,null,"土間下砕石撤去",null,0.1,"㎥"]
[]
[6,null,"既設コンクリート面目荒し","H=200",0.8,"㎡"]
[]
[7]
[]
[8]
[]
[9,"（内部）","天井石膏ボード撤去","t=9.5",4.2,"㎡"]
[]
[10,null,"天井岩綿吸音板撤去","下地共",7.7,"㎡"]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"5　の計"]
[]
[1]
[]
[2,6,"発生材積込運搬費"]
[]
[3,null,"発生材積込費"]
[]
[4,null,"がれき類",null,0.2,"㎥"]
[]
[5,null,"ボード類",null,0.3,"㎥"]
[]
[6]
[]
[7]
[]
[8,null,"発生材運搬費"]
[]
[9,null,"移動式コンテナ","8tコンテナ車",1,"回"]
[]
[10]
[]
[11]
[]
[12,null,null,null," "]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"6　の計"]
[]
[1]
[]
[2,7,"発生材処分費"]
[]
[3,null,"発生材処分"]
[]
[4,null,"がれき類",null,0.2,"㎥"]
[]
[5,null,"ボード類",null,0.3,"㎥"]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"7　の計"]
[]
[1,null,null,null," "]
[]
[2,"Ⅱ","改修電気設備工事"]
[]
[3,1,"電灯設備工事",null,1,"式"]
[]
[4,2,"動力設備工事",null,1,"式"]
[]
[5,3,"弱電設備工事",null,1,"式"]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"2　の計"]
[]
[1,null,null,null," "]
[]
[2,1,"電灯設備工事"]
[]
[3,null,"電線","EM-EEF2.0-2C　コロガシ",3,"ｍ"]
[]
[4,null,"電線","EM-EEF2.0-3C　コロガシ",49,"ｍ"]
[]
[5,null,"メタルモールジング","A型",2,"ｍ"]
[]
[6,null,"ボックス類",null,1,"式"]
[]
[7,null,"既設電灯盤改造費","L-1-1",1,"式"]
[]
[8,null,"既設電灯盤改造費","L-1-2",1,"式"]
[]
[9,null,"既設電灯盤改造費","L-2",1,"式"]
[]
[10,null,"撤去工事費",null,1,"式"]
[]
[11,null,"移設工事費",null,1,"式"]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"1　の計"]
[]
[1,null,null,null," "]
[]
[2,2,"動力設備工事"]
[]
[3,null,"電線管","HI(22)　露出",25,"ｍ"]
[]
[4,null,"電線管","HI(28)　露出",23,"ｍ"]
[]
[5,null,"電線管","HI(54)　露出",2,"ｍ"]
[]
[6,null,"電線","EM-E 14ﾟ　管内",2,"ｍ"]
[]
[7,null,"電線","EM-CE5.5ﾟ-4C　管内",23,"ｍ"]
[]
[8,null,"電線","EM-CET22ﾟ　管内",2,"ｍ"]
[]
[9,null,"電線","EM-CEE-S1.25ﾟ-2C　管内",25,"ｍ"]
[]
[10,null,"動力分電盤","1M-AC　屋外自立型",1,"面"]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"2　の計"]
[]
[1,null,null,null," "]
[]
[2,3,"弱電設備工事"]
[]
[3,null,"電線","AE1.2-4C　コロガシ",3,"ｍ"]
[]
[4,null,"電線","HP1.2-3C　コロガシ",3,"ｍ"]
[]
[5,null,"移設工事費",null,1,"式"]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"3　の計"]
[]
[1,null,null,null," "]
[]
[2,"Ⅲ","改修機械設備工事"]
[]
[3,1,"機器設備工事",null,1,"式"]
[]
[4,2,"配管設備工事",null,1,"式"]
[]
[5,3,"空調ダクト設備工事",null,1,"式"]
[]
[6,4,"ガス設備工事",null,1,"式"]
[]
[7,5,"消火設備工事",null,1,"式"]
[]
[8,6,"撤去工事",null,1,"式"]
[]
[9,7,"発生材処理",null,1,"式"]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"3　の計"]
[]
[1,null,null,null," "]
[]
[2,1,"機器設備工事"]
[null,null,"GHP-1ガスヒ－トポンプ式","室外機"]
[3,null,"マルチエアコン","冷房能力：56.0ｋｗ、暖房能力：63.0ｋｗ　付属品共",1,"台"]
[null,null,"GHP1-1ガスヒ－トポンプ式","室内機　壁掛形"]
[4,null,"マルチエアコン","冷房能力：3.6ｋｗ、暖房能力：4.0ｋｗ　付属品共",1,"台"]
[]
[5,null,"ワイヤ－ドリモコンスイッチ",null,1,"個"]
[null,null,"GHP1-2ガスヒ－トポンプ式","室内機　天井カセット4方向吹出"]
[6,null,"マルチエアコン","冷房能力：7.1ｋｗ、暖房能力：8.0ｋｗ　付属品共",1,"台"]
[]
[7,null,"ワイヤ－ドリモコンスイッチ",null,1,"個"]
[null,null,"GHP1-3ガスヒ－トポンプ式","室内機　壁掛形"]
[8,null,"マルチエアコン","冷房能力：4.5ｋｗ、暖房能力：5.0ｋｗ　付属品共",1,"台"]
[]
[9,null,"ワイヤ－ドリモコンスイッチ",null,1,"個"]
[null,null,"GHP1-4ガスヒ－トポンプ式","室内機　天井カセット2方向吹出"]
[10,null,"マルチエアコン","冷房能力：7.1ｋｗ、暖房能力：8.0ｋｗ　付属品共",2,"台"]
[]
[11,null,"ワイヤ－ドリモコンスイッチ",null,1,"個"]
[null,null,"GHP1-5ガスヒ－トポンプ式","室内機　天井カセット2方向吹出"]
[12,null,"マルチエアコン","冷房能力：7.1ｋｗ、暖房能力：8.0ｋｗ　付属品共",2,"台"]
[]
[13,null,"ワイヤ－ドリモコンスイッチ",null,1,"個"]
[null,null,"GHP1-6ガスヒ－トポンプ式","室内機　天井埋込ダクト形"]
[14,null,"マルチエアコン","冷房能力：14.0ｋｗ、暖房能力：16.0ｋｗ　付属品共",1,"台"]
[]
[15,null,"ワイヤ－ドリモコンスイッチ",null,1,"個"]
[null,null,"GHP-2ガスヒ－トポンプ式","室外機"]
[16,null,"マルチエアコン","冷房能力：45.0ｋｗ、暖房能力：50.0ｋｗ　付属品共",1,"台"]
[null,null,"GHP2-1ガスヒ－トポンプ式","室内機　天井カセット2方向吹出"]
[17,null,"マルチエアコン","冷房能力：4.5ｋｗ、暖房能力：5.0ｋｗ　付属品共",6,"台"]
[]
[18,null,"ワイヤ－ドリモコンスイッチ",null,2,"個"]
[null,null,"GHP2-2ガスヒ－トポンプ式","室内機　天井カセット2方向吹出"]
[19,null,"マルチエアコン","冷房能力：5.6ｋｗ、暖房能力：6.3ｋｗ　付属品共",1,"台"]
[]
[20]
[]
[1]
[]
[2,null,"ワイヤ－ドリモコンスイッチ",null,1,"個"]
[null,null,"GHP2-3ガスヒ－トポンプ式","室内機　天井カセット2方向吹出"]
[3,null,"マルチエアコン","冷房能力：7.1ｋｗ、暖房能力：8.0ｋｗ　付属品共",1,"台"]
[]
[4,null,"ワイヤ－ドリモコンスイッチ",null,1,"個"]
[null,null,"GHP-3ガスヒ－トポンプ式","室外機"]
[5,null,"マルチエアコン","冷房能力：85.0ｋｗ、暖房能力：95.0ｋｗ　付属品共",1,"台"]
[null,null,"GHP3-1ガスヒ－トポンプ式","室内機　天井埋込ダクト形"]
[6,null,"マルチエアコン","冷房能力：5.6ｋｗ、暖房能力：6.3ｋｗ　付属品共",6,"台"]
[]
[7,null,"ワイヤ－ドリモコンスイッチ",null,2,"個"]
[null,null,"GHP3-2ガスヒ－トポンプ式","室内機　床置ローボーイ埋込形"]
[8,null,"マルチエアコン","冷房能力：4.5ｋｗ、暖房能力：5.0ｋｗ　付属品共",6,"台"]
[]
[9,null,"ワイヤ－ドリモコンスイッチ",null,2,"個"]
[null,null,"GHP3-3ガスヒ－トポンプ式","室内機　天井埋込ﾀﾞｸﾄ形"]
[10,null,"マルチエアコン","冷房能力：9.0ｋｗ、暖房能力：10.0ｋｗ　付属品共",2,"台"]
[null,null,"GHP3-4ガスヒ－トポンプ式","室内機　天井埋込ﾀﾞｸﾄ形"]
[11,null,"マルチエアコン","冷房能力：4.5ｋｗ、暖房能力：5.0ｋｗ　付属品共",1,"台"]
[]
[12,null,"ワイヤ－ドリモコンスイッチ",null,1,"個"]
[null,null,"GHP-4ガスヒ－トポンプ式","室外機"]
[13,null,"マルチエアコン","冷房能力：56.0ｋｗ、暖房能力：63.0ｋｗ　付属品共",1,"台"]
[null,null,"GHP4-1ガスヒ－トポンプ式","室内機　天井埋込ﾀﾞｸﾄ形"]
[14,null,"マルチエアコン","冷房能力：9.0ｋｗ、暖房能力：10.0ｋｗ　付属品共",1,"台"]
[]
[15,null,"ワイヤ－ドリモコンスイッチ",null,1,"個"]
[null,null,"GHP4-2ガスヒ－トポンプ式","室内機　天井ｶｾｯﾄ2方向吹出"]
[16,null,"マルチエアコン","冷房能力：4.5ｋｗ、暖房能力：5.0ｋｗ　付属品共",2,"台"]
[]
[17,null,"ワイヤ－ドリモコンスイッチ",null,1,"個"]
[null,null,"GHP4-3ガスヒ－トポンプ式","室内機　天井ｶｾｯﾄ2方向吹出"]
[18,null,"マルチエアコン","冷房能力：4.5ｋｗ、暖房能力：5.0ｋｗ　付属品共",2,"台"]
[]
[19,null,"ワイヤ－ドリモコンスイッチ",null,1,"個"]
[]
[20]
[]
[1,null,null,null," "]
[null,null,"GHP4-4ガスヒ－トポンプ式","室内機　天井ｶｾｯﾄ2方向吹出"]
[2,null,"マルチエアコン","冷房能力：4.5ｋｗ、暖房能力：5.0ｋｗ　付属品共",2,"台"]
[]
[3,null,"ワイヤ－ドリモコンスイッチ",null,1,"個"]
[null,null,"GHP4-5ガスヒ－トポンプ式","室内機　天井ｶｾｯﾄ2方向吹出"]
[4,null,"マルチエアコン","冷房能力：4.5ｋｗ、暖房能力：5.0ｋｗ　付属品共",2,"台"]
[]
[5,null,"ワイヤ－ドリモコンスイッチ",null,1,"個"]
[null,null,"GHP4-6ガスヒ－トポンプ式","室内機　天井ｶｾｯﾄ2方向吹出"]
[6,null,"マルチエアコン","冷房能力：4.5ｋｗ、暖房能力：5.0ｋｗ　付属品共",2,"台"]
[]
[7,null,"ワイヤ－ドリモコンスイッチ",null,1,"個"]
[]
[8,null,"集中管理リモコンスイッチ",null,1,"個"]
[]
[9,null,"遠隔監視アダプタ－",null,1,"個"]
[]
[10,null,"冷媒ｶﾞｽ漏れ検知器",null,13,"個"]
[]
[11,null,"機器搬入費",null,1,"式"]
[]
[12,null,"機器固定アンカーボルト",null,1,"式"]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"1　の計"]
[]
[1]
[]
[2,2,"配管設備工事"]
[]
[3,null,"冷媒用保温付被覆銅管","ガス管保温厚20mm：12.7φ",99,"ｍ"]
[]
[4,null,"冷媒用保温付被覆銅管","ガス管保温厚20mm：15.9φ",102,"ｍ"]
[]
[5,null,"冷媒用保温付被覆銅管","ガス管保温厚20mm：22.2φ",29,"ｍ"]
[]
[6,null,"冷媒用保温付被覆銅管","ガス管保温厚20mm：28.6φ",105,"ｍ"]
[]
[7,null,"冷媒用保温付被覆銅管","ガス管保温厚20mm：31.8φ",49,"ｍ"]
[]
[8,null,"冷媒用保温付被覆銅管","液管保温厚8mm：6.4φ",99,"ｍ"]
[]
[9,null,"冷媒用保温付被覆銅管","液管保温厚8mm：9.5φ",131,"ｍ"]
[]
[10,null,"冷媒用保温付被覆銅管","液管保温厚10mm：12.7φ",29,"ｍ"]
[]
[11,null,"冷媒用保温付被覆銅管","液管保温厚10mm：15.9φ",75,"ｍ"]
[]
[12,null,"冷媒用保温付被覆銅管","液管保温厚10mm：19.1φ",49,"ｍ"]
[]
[13,null,"結露防止用保温付ポリ塩化ビニル管","25A　屋内露出・隠蔽",65,"ｍ"]
[]
[14,null,"硬質ポリ塩化ビニル管","20A　屋外露出",3,"ｍ"]
[]
[15,null,"硬質ポリ塩化ビニル管","50A　屋外露出",6,"ｍ"]
[]
[16,null,"既設配管接続費",null,1,"式"]
[]
[17,null,"はつり及び補修",null,1,"式"]
[]
[18,null,"保温工事",null,1,"式"]
[]
[19,null,"連絡配線・リモコン配線工事",null,1,"式"]
[]
[20]
[]
[1,null,null,null," "]
[]
[2,null,"配管架台",null,1,"式"]
[]
[3]
[]
[4]
[]
[5]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"2　の計"]
[]
[1,null,null,null," "]
[]
[2,3,"空調ダクト設備工事"]
[]
[3,null,"器具取外し再取付費",null,1,"式"]
[]
[4,null,"たわみ継手",null,1,"式"]
[]
[5,null,"既設ダクト接続費",null,1,"式"]
[]
[6,null,"天井開口及び補強",null,1,"式"]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"3　の計"]
[]
[1,null,null,null," "]
[]
[2,4,"ガス設備工事"]
[]
[3,null,"ガス露出配管","被覆鋼管　PLS-50A",8,"ｍ"]
[]
[4,null,"ガス露出配管","被覆鋼管　PLS-20A",4,"ｍ"]
[]
[5,null,"同上継手",null,1,"式"]
[]
[6,null,"雑材料",null,1,"式"]
[]
[7,null,"メーターガス栓","50A",2,"個"]
[]
[8,null,"ハンドガス栓（検圧孔付）","20A",4,"個"]
[]
[9,null,"強化ホース巻","20mm",2,"ｍ"]
[]
[10,null,"強化ホース接続金具","20mm",4,"組"]
[]
[11,null,"検圧プラグ","F910B",1,"個"]
[]
[12,null,"配管工事",null,1,"式"]
[]
[13,null,"管支持金具取付工費",null,1,"式"]
[]
[14,null,"機器接続工費",null,1,"式"]
[null,null,"ガスメーター特殊部材及び"]
[15,null,"ガスメーター廻り配管更新工事",null,1,"式"]
[]
[16,null,"既設配管切り離し撤去工事",null,1,"式"]
[]
[17,null,"材料運搬費",null,1,"式"]
[]
[18,null,"現場管理費",null,1,"式"]
[]
[19,null,"法定福利費",null,1,"式"]
[]
[20]
[]
[1,null,null,null," "]
[]
[2]
[]
[3]
[]
[4]
[]
[5]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"4　の計"]
[]
[1,null,null,null," "]
[]
[2,5,"消火設備工事"]
[]
[3,null,"消火器","粉末消火器ABC10型",2,"個"]
[]
[4,null,"消火器屋外設置箱",null,2,"個"]
[]
[5]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"5　の計"]
[]
[1,null,null,null," "]
[]
[2,6,"撤去工事"]
[]
[3,null,"空調機撤去","搬出費含む",1,"式"]
[]
[4,null,"冷媒ガス回収・破壊費",null,1,"式"]
[]
[5,null,"配管類撤去","保温撤去含む",1,"式"]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"6　の計"]
[]
[1,null,null,null," "]
[]
[2,7,"発生材処理"]
[]
[3,null,"発生材積込",null,1,"式"]
[]
[4,null,"発生材運搬",null,1,"式"]
[]
[5,null,"発生材処分（スクラップ）","鉄　ヘビーH2　（5.39t）",1,"式"]
[]
[6]
[]
[7]
[]
[8]
[]
[9]
[]
[10]
[]
[11]
[]
[12]
[]
[13]
[]
[14]
[]
[15]
[]
[16]
[]
[17]
[]
[18]
[]
[19]
[]
[20,null,"7　の計"]