{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["表紙","設計書"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":4,"defined_names":21,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"表紙","index":0,"n_rows":24,"n_cols":10,"rows_kept":24,"cut":false,"hidden":false,"merged":[[16,6,18,10],[33,5,34,10],[20,0,22,4],[16,0,19,0],[16,3,19,4],[16,5,18,5],[23,6,25,7],[23,8,25,8],[42,5,43,10],[39,5,41,10],[37,5,38,10],[19,5,22,5],[19,8,22,8],[35,5,36,10],[31,5,32,10],[29,5,30,10],[27,5,28,10],[23,5,25,5],[19,6,22,7],[23,9,25,10],[19,9,22,10],[23,0,43,4],[0,0,3,0],[8,0,11,0],[4,0,7,0],[14,3,15,3],[8,3,11,4],[12,1,13,1],[14,1,15,1],[12,0,15,0],[8,1,11,1],[12,2,13,2],[8,2,11,2],[14,2,15,2],[16,1,19,2],[8,5,11,5],[0,1,3,10],[4,1,7,10],[14,4,15,10],[12,3,13,3],[12,4,13,10]]}
["令和3年度","工　　 事　　 設　　 計　　 書"]
[]
[]
[]
["工　 事   名","依那古小学校統合改修工事（建築主体工事）"]
[]
[]
[]
["施 工 地 名",null,"伊賀市","沖",null,"地内"]
[]
[]
[]
["工       費"]
[]
[null,"\\"]
[]
["工       期","本契約日の翌日から　　",null,"令和４年10月28日まで",null,"設　計","令和４年１月"]
[]
[]
[null,null,null,null,null,"設　計",null,null,"検　算"]
["工　　事　　の　　大　　要"]
[]
[]
["依那古小学校、神戸小学校、比自岐小学校（休校）の統合に伴う改修工事（建築主体工事）\n\n①校舎　鉄筋コンクリート造３階建　2,395㎡\n　防水改修工事　一式、外壁改修工事　一式、建具改修工事　一式、内装改修工事　一式、塗装改修工事　一式、躯体改修工事　一式　ほか\n\n②屋内運動場　鉄骨造１階建　563㎡\n　外壁改修工事　一式、建具改修工事　一式、内装改修工事　一式、塗装改修工事　一式　ほか\n\n③外構\n　門扉工事　一式、駐車場工事　一式　ほか",null,null,null,null,"業　種","建",null,"業種コード","02"]

{"sheet":"設計書","index":1,"n_rows":1943,"n_cols":8,"rows_kept":1943,"cut":false,"hidden":false,"merged":[[126,7,126,16],[167,7,167,16],[153,7,153,16],[422,7,422,16],[159,7,159,16],[160,7,160,16],[161,7,161,16],[162,7,162,16],[163,7,163,16],[164,7,164,16],[469,27,469,36],[129,7,129,16],[468,27,468,36],[239,7,239,16],[240,7,240,16],[0,1,0,2],[4,13,4,16],[75,7,75,9],[110,7,110,16],[133,7,133,16],[123,7,123,16],[128,7,128,16],[130,7,130,16],[125,7,125,16],[115,7,115,16],[127,7,127,16],[124,7,124,16],[144,7,144,16],[155,7,155,16],[156,7,156,16],[157,7,157,16],[158,7,158,16],[121,7,121,16],[122,7,122,16],[75,10,75,12],[75,13,75,14],[75,15,75,16],[76,7,76,8],[76,10,76,11],[76,13,76,14],[76,15,76,16],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[17,15,17,16],[1,5,2,5],[1,6,2,6],[1,7,2,16],[4,7,4,11],[77,7,77,9],[77,10,77,12],[77,13,77,14],[77,15,77,16],[95,7,95,9],[95,10,95,12],[95,13,95,14],[95,15,95,16],[96,7,96,8],[96,10,96,11],[96,13,96,14],[96,15,96,16],[79,7,79,9],[79,10,79,12],[79,13,79,14],[79,15,79,16],[81,7,81,9],[81,10,81,12],[81,13,81,14],[81,15,81,16],[83,7,83,9],[83,10,83,12],[83,13,83,14],[83,15,83,16],[97,7,97,9],[97,10,97,12],[97,13,97,14],[97,15,97,16],[86,7,86,8],[86,10,86,11],[86,13,86,14],[86,15,86,16],[87,7,87,9],[87,10,87,12],[87,13,87,14],[87,15,87,16],[92,7,92,8],[92,10,92,11],[92,13,92,14],[92,15,92,16],[93,7,93,9],[94,7,94,8],[94,10,94,11],[94,13,94,14],[94,15,94,16],[93,10,93,12],[93,13,93,14],[93,15,93,16],[85,7,85,9],[85,10,85,12],[85,13,85,14],[85,15,85,16],[90,7,90,8],[90,10,90,11],[90,13,90,14],[90,15,90,16],[91,7,91,9],[91,10,91,12],[91,13,91,14],[91,15,91,16],[88,7,88,8],[88,10,88,11],[88,13,88,14],[88,15,88,16],[89,7,89,9],[89,10,89,12],[89,13,89,14],[89,15,89,16]]}
[null,"依那古小学校統合改修工事（建築主体工事）"]
["用途","名　　称","摘　　　　要","数    量","単位","単    価","金    額","備　　　考"]
[]
[]
["Ａ","直接工事費","発生材処分費共",1,"式"]
[]
[]
[]
["Ｂ","共通仮設費","共通仮設費率",1,"式"]
[]
[null,"共通仮設費","積み上げ",1,"式"]
[]
[]
[]
[null,"純工事費"]
[]
[]
[]
["Ｃ","現場管理費","現場管理費率",1,"式"]
[]
[]
[]
[]
[]
[null,"工事原価"]
[]
[]
[]
["Ｄ","一般管理費",null,1,"式"]
[]
[]
[]
[null,"工事価格"]
[]
[]
[]
[null,"消費税及び地方消費税",null,1,"式"]
[]
[]
[]
[null,"工事費計"]
[]
["A","直接工事費"]
[]
["a","校舎改修工事",null,1,"式"]
[]
["b","屋内運動場改修工事",null,1,"式"]
[]
["c","外構工事",null,1,"式"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"A　　　計"]
[]
[]
[]
["a","校舎改修工事"]
[]
[1,"(校舎)直接仮設工事",null,1,"式"]
[]
[2,"(校舎)防水改修工事",null,1,"式"]
[]
[3,"(校舎)外壁改修工事",null,1,"式"]
[]
[4,"(校舎)建具改修工事",null,1,"式"]
[]
[5,"(校舎)内装改修工事",null,1,"式"]
[]
[6,"(校舎)塗装改修工事",null,1,"式"]
[]
[7,"(校舎)躯体改修工事",null,1,"式"]
[]
[8,"(校舎)環境配慮改修工事",null,1,"式"]
[]
[9,"(校舎)発生材積込運搬費",null,1,"式"]
[]
[10,"(校舎)発生材処分費",null,1,"式"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"a　計"]
[]
[]
["a"]
[1,"(校舎)直接仮設工事"]
[]
[null,"（ 外 部 ）"]
[]
[null,"枠組み本足場","手摺先行方式　W900",2747,"m2"]
[]
[null,"枠組み本足場","手摺先行方式　W600",33.799999999999997,"m2"]
[]
[null,"養生シート","ﾒｯｼｭｼｰﾄ",2814,"m2"]
[]
[null,"ブラケット足場",null,66,"m2"]
[]
[null,"安全手摺",null,44,"ｍ"]
[null,"ﾍﾞﾗﾝﾀﾞ"]
[null,"枠組み本足場","手摺先行方式　W900",450,"m2"]
[null,"ﾍﾞﾗﾝﾀﾞ"]
[null,"枠組み本足場","手摺先行方式　W600",134,"m2"]
[]
[]
[null,"防水改修"]
[null,"養生",null,1345,"m2"]
[null,"防水改修"]
[null,"整理清掃後片付け",null,1345,"m2"]
[]
[]
[null,"外壁改修"]
[null,"養生",null,372,"m2"]
[null,"外壁改修"]
[null,"整理清掃後片付け",null,372,"m2"]
[]
[]
[]
[]
[]
[]
[]
[null,"（ 内 部 ）"]
[null,"内装改修"]
[null,"墨出し",null,757,"m2"]
[null,"内装改修"]
[null,"養生",null,757,"m2"]
[null,"内装改修"]
[null,"整理清掃後片付け",null,757,"m2"]
[null,"内装改修"]
[null,"内部足場","脚立",267,"m2"]
[null,"内装改修"]
[null,"階段足場",null,96,"m2"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"a-１　計"]
[]
[]
["a"]
[2,"(校舎)防水改修工事"]
[]
[null,"（ 撤 去 ）"]
[null,"屋根平場"]
[null,"目地材撤去",null,376,"ｍ"]
[null,"屋根平場"]
[null,"既設ドレン撤去","100φ",8,"か所"]
[]
[]
[null,"東ﾍﾞﾗﾝﾀﾞ床"]
[null,"目地カッター切り",null,163,"ｍ"]
[null,"東ﾍﾞﾗﾝﾀﾞ床"]
[null,"目地材撤去",null,81.5,"ｍ"]
[]
[]
[null,"西ﾍﾞﾗﾝﾀﾞ床"]
[null,"アスファルト防水撤去",null,69.3,"m2"]
[null,"西ﾍﾞﾗﾝﾀﾞ床"]
[null,"目地材撤去",null,29,"ｍ"]
[null,"西ﾍﾞﾗﾝﾀﾞ立上り"]
[null,"既設防水層撤去",null,10,"m2"]
[null,"西ﾍﾞﾗﾝﾀﾞ立上り"]
[null,"押え金物撤去",null,36.5,"ｍ"]
[null,"西ﾍﾞﾗﾝﾀﾞ立上り"]
[null,"シーリング撤去",null,36.5,"ｍ"]
[]
[]
[null,"ﾍﾞﾗﾝﾀﾞ"]
[null,"既設ドレン撤去",null,10,"か所"]
[null,"ﾍﾞﾗﾝﾀﾞ"]
[null,"既設目皿撤去",null,3,"か所"]
[null,"ﾍﾞﾗﾝﾀﾞ"]
[null,"既設中継ドレン撤去",null,8,"か所"]
[]
[null,"( 改 修 )"]
[null,"屋根平場"]
[null,"高圧水洗浄","10～15Mpa",832,"m2"]
[null,"屋根平場"]
[null,"エポキシ系ポリマーセメント",null,832,"m2"]
[null,"屋根平場"]
[null,"ウレタン塗膜防水","X-1",832,"m2"]
[null,"屋根平場"]
[null,"目地テープ処理",null,376,"ｍ"]
[null,"屋根平場"]
[null,"凹凸部ケレン掛け平滑処理",null,101,"m2"]
[null,"屋根立上り"]
[null,"高圧水洗浄","10～15Mpa",198,"m2"]
[null,"屋根立上り"]
[null,"エポキシ系ポリマーセメント",null,198,"m2"]
[null,"屋根立上り"]
[null,"ウレタン塗膜防水","X-2",198,"m2"]
[null,"屋根立上り"]
[null,"防水端末シーリング","MS-2",86,"ｍ"]
[null,"屋根平場"]
[null,"脱気筒","SUS",10,"か所"]
[null,"屋根平場"]
[null,"改修用ルーフドレン","100φ",7,"か所"]
[null,"屋根平場"]
[null,"改修用横引ドレン","100φ",1,"か所"]
[null,"屋根平場"]
[null,"ドレン廻り修正",null,8,"か所"]
[]
[]
[null,"ﾍﾞﾗﾝﾀﾞ床"]
[null,"高圧水洗浄","10～15Mpa",272,"m2"]
[null,"ﾍﾞﾗﾝﾀﾞ床"]
[null,"エポキシ系ポリマーセメント",null,272,"m2"]
[null,"ﾍﾞﾗﾝﾀﾞ床"]
[null,"塗膜防水","X-2",272,"m2"]
[null,"ﾍﾞﾗﾝﾀﾞ立上り"]
[null,"高圧水洗浄","10～15Mpa",88.4,"m2"]
[null,"ﾍﾞﾗﾝﾀﾞ立上り"]
[null,"エポキシ系ポリマーセメント",null,88.4,"m2"]
[null,"ﾍﾞﾗﾝﾀﾞ立上り"]
[null,"塗膜防水","X-2",88.4,"m2"]
[null,"ﾍﾞﾗﾝﾀﾞ"]
[null,"防水端末シーリング","MS-2",528,"ｍ"]
[null,"ﾍﾞﾗﾝﾀﾞ"]
[null,"既設室外機一時撤去復旧",null,4,"か所"]
[]
[]
[null,"西ﾍﾞﾗﾝﾀﾞ床"]
[null,"高圧水洗浄","10～15Mpa",69.3,"m2"]
[null,"西ﾍﾞﾗﾝﾀﾞ床"]
[null,"エポキシ系ポリマーセメント",null,69.3,"m2"]
[null,"西ﾍﾞﾗﾝﾀﾞ床"]
[null,"塗膜防水 X-1","X-1",69.3,"m2"]
[null,"西ﾍﾞﾗﾝﾀﾞ立上り"]
[null,"高圧水洗浄","10～15Mpa",10.6,"m2"]
[null,"西ﾍﾞﾗﾝﾀﾞ立上り"]
[null,"エポキシ系ポリマーセメント",null,10.6,"m2"]
[null,"西ﾍﾞﾗﾝﾀﾞ立上り"]
[null,"塗膜防水","X-2",10.6,"m2"]
[null,"西ﾍﾞﾗﾝﾀﾞ床"]
[null,"目地テープ処理",null,29,"ｍ"]
[null,"西ﾍﾞﾗﾝﾀﾞ床"]
[null,"目地ケレン清掃",null,29,"ｍ"]
[null,"西ﾍﾞﾗﾝﾀﾞ立上り"]
[null,"ケレン清掃",null,36.5,"ｍ"]
[]
[]
[null,"東ﾍﾞﾗﾝﾀﾞ床"]
[null,"高圧水洗浄","10～15Mpa",172,"m2"]
[null,"東ﾍﾞﾗﾝﾀﾞ床"]
[null,"エポキシ系ポリマーセメント",null,172,"m2"]
[null,"東ﾍﾞﾗﾝﾀﾞ床"]
[null,"塗膜防水","X-1",172,"m2"]
[null,"東ﾍﾞﾗﾝﾀﾞ立上り"]
[null,"高圧水洗浄","10～15Mpa",27.1,"m2"]
[null,"東ﾍﾞﾗﾝﾀﾞ立上り"]
[null,"エポキシ系ポリマーセメント",null,27.1,"m2"]
[null,"東ﾍﾞﾗﾝﾀﾞ立上り"]
[null,"塗膜防水","X-2",27.1,"m2"]
[null,"東ﾍﾞﾗﾝﾀﾞ床"]
[null,"目地テープ処理",null,81.5,"ｍ"]
[null,"東ﾍﾞﾗﾝﾀﾞ床"]
[null,"目地ケレン清掃",null,81.5,"ｍ"]
[]
[]
[null,"ﾍﾞﾗﾝﾀﾞ"]
[null,"改修用ルーフドレン","100φ",8,"か所"]
[null,"ﾍﾞﾗﾝﾀﾞ"]
[null,"改修用横引ドレン","100φ",2,"か所"]
[null,"ﾍﾞﾗﾝﾀﾞ"]
[null,"目皿","100φ",3,"か所"]
[null,"ﾍﾞﾗﾝﾀﾞ"]
[null,"改修用中継ドレン","100φ",8,"か所"]
[null,"ﾍﾞﾗﾝﾀﾞ"]
[null,"ドレン廻り修正",null,21,"か所"]
[null,"ﾍﾞﾗﾝﾀﾞ"]
[null,"脱気筒",null,3,"か所"]
[]
[null,"a-2　計"]
[]
[]
["a"]
[3,"(校舎)外壁改修工事"]
[]
[null,"（ 撤 去 ）"]
[null,"玄関"]
[null,"床マット撤去","W1700×D500",1,"か所"]
[null,"玄関"]
[null,"樹脂製校章撤去",null,1,"か所"]
[null,"玄関校歌石碑"]
[null,"基礎コンクリート撤去","ﾊﾝﾄﾞﾌﾞﾚｰｶｰ",0.2,"m3"]
[null,"玄関床"]
[null,"土間コンクリートカッター切り",null,13,"ｍ"]
[null,"玄関床"]
[null,"土間砕石撤去",null,1,"m3"]
[null,"玄関床"]
[null,"土間コン撤去",null,1.5,"m3"]
[null,"玄関床"]
[null,"モルタルカッター切り",null,2.8,"ｍ"]
[null,"玄関床"]
[null,"タイル撤去",null,17.8,"m2"]
[null,"玄関壁"]
[null,"モルタルカッター切り",null,3.6,"ｍ"]
[null,"玄関壁"]
[null,"建築記念銘板撤去","W1000×H800",1,"か所"]
[]
[null,"（ 改 修 ）"]
[]
[null,"外壁事前調査",null,2009,"㎡"]
[null,"外壁"]
[null,"水洗い","高圧ポンプによる水洗い程度",2009,"㎡"]
[null,"外壁"]
[null,"外壁補修",null,1,"式"]
[null,"外壁"]
[null,"外壁用塗膜防水材","下地調整共",2009,"m2"]
[]
[]
[null,"玄関"]
[null,"校章","取付費共",1,"か所"]
[]
[]
[null,"玄関床"]
[null,"モルタル塗り","ﾀｲﾙ下地",21.3,"m2"]
[null,"ｽﾛｰﾌﾟ床"]
[null,"モルタル塗り","ﾀｲﾙ下地",6.6,"m2"]
[null,"玄関床"]
[null,"磁器質タイル","150角",18.8,"m2"]
[null,"玄関床"]
[null,"点状タイル","300角",2.5,"m2"]
[null,"ｽﾛｰﾌﾟ床"]
[null,"磁器質タイル","150角 識別しやすい色",6.6,"m2"]
[null,"玄関"]
[null,"段鼻タイル",null,8.9,"ｍ"]
[null,"玄関立上り"]
[null,"打放し補修","吹付下地",7.7,"m2"]
[null,"玄関立上り天端"]
[null,"コンクリート金鏝押え","W150 吹付下地",12.8,"ｍ"]
[null,"玄関立上り"]
[null,"複層塗材Ｅ","RC面 天端含む",9.6,"m2"]
[null,"玄関"]
[null,"手摺","SUS 2段 H500 既製品",1,"式"]
[null,"玄関壁"]
[null,"モルタル塗り","館名板撤去跡　ﾀｲﾙ下地",0.8,"m2"]
[null,"玄関壁"]
[null,"小口タイル","館名板撤去跡",0.8,"m2"]
[]
[null,"a-3　計"]
[]
[]
["a"]
[4,"(校舎)建具改修工事"]
[]
[null,"（ 撤 去 ）"]
[]
[null,"建具廻りカッター切",null,91.2,"ｍ"]
[]
[null,"溝斫り",null,45.6,"ｍ"]
[]
[null,"アルミ建具撤去","両開き 枠残し",237,"m2"]
[]
[null,"アルミ建具撤去","両開き 枠共",21.6,"m2"]
[]
[null,"トイレブース撤去",null,95.7,"m2"]
[]
[null,"木製建具撤去","片開き 枠残し",1.8,"m2"]
[]
[null,"建具廻りシーリング撤去",null,712,"ｍ"]
[]
[null,"ガラス撤去","t3",244,"m2"]
[]
[null,"（ 改 修 ）","運搬取付調整共"]
[null,"ADW-2"]
[null,"網戸","850×1200",21,"か所"]
[null,"AW-3"]
[null,"網戸","900×1200",4,"か所"]
[]
[]
[null,"AW-1","ｶﾊﾞｰ工法"]
[null,"引違い段窓連窓アルミサッシ","2970×2205",1,"か所"]
[null,"AW-3","ｶﾊﾞｰ工法･ｱﾙﾐﾊﾟﾈﾙ共"]
[null,"引違い段窓連窓アルミサッシ","3290×2205",1,"か所"]
[null,"AW-3","ｶﾊﾞｰ工法"]
[null,"引違い段窓連窓アルミサッシ","3290×2205",1,"か所"]
[null,"AW-8","ｶﾊﾞｰ工法"]
[null,"引違い段窓連窓アルミサッシ","3390×2205",2,"か所"]
[null,"AW-10","ｶﾊﾞｰ工法･ｱﾙﾐﾊﾟﾈﾙ共"]
[null,"引違い段窓連窓アルミサッシ","7230×1905",1,"か所"]
[null,"AW-10","ｶﾊﾞｰ工法"]
[null,"引違い段窓連窓アルミサッシ","7230×1905",5,"か所"]
[null,"AW-11","ｶﾊﾞｰ工法･ｱﾙﾐﾊﾟﾈﾙ共"]
[null,"引違い段窓連窓アルミサッシ","3390×1905",4,"か所"]
[null,"AW-11","ｶﾊﾞｰ工法"]
[null,"引違い段窓連窓アルミサッシ","3390×1905",6,"か所"]
[null,"AW-13","ｶﾊﾞｰ工法"]
[null,"引違い段窓連窓アルミサッシ","3290×1905",1,"か所"]
[null,"AD-1","ｶﾊﾞｰ工法"]
[null,"両開きガラスドア","1800×2000",1,"か所"]
[]
[null,"以上取付調整費",null,1,"式"]
[null,"AD-5","ｱﾙﾐｶﾞﾗﾘ新設"]
[null,"アルミガラリ","680×400",1,"か所"]
[]
[null,"以上取付調整費",null,1,"式"]
[null,"HD-1","ｱﾙﾐｶﾞﾗﾘ付"]
[null,"片引き自閉式ハンガー戸","1020×2000　取付調整費共",1,"か所"]
[null,"SD-3"]
[null,"ｽﾁｰﾙ点検扉","400×400　取付調整費共",3,"か所"]
[]
[]
[null,"TB-1"]
[null,"トイレブース","(1140+500+2700)×2000　取付費共",3,"か所"]
[null,"TB-2"]
[null,"トイレブース","(340+940)×2000　取付費共",1,"か所"]
[null,"TB-3"]
[null,"トイレブース","900×2000　取付費共",1,"か所"]
[null,"TB-4"]
[null,"トイレブース","(1230×2+1840)×2000　取付費共",2,"か所"]
[null,"TB-5"]
[null,"トイレブース","(1230×2+1840)×2000　取付費共",2,"か所"]
[]
[]
[null,"FD-1","ｱﾙﾐｶﾞﾗﾘ付"]
[null,"片開きフラッシュドア","800×2000",3,"か所"]
[null,"FD-2","ｱﾙﾐｶﾞﾗﾘ付"]
[null,"片開きフラッシュドア","800×2000",3,"か所"]
[null,"WD-1","枠ﾚｰﾙは再利用"]
[null,"片引きフラッシュ戸","900×2000",18,"か所"]
[]
[null,"以上搬入取付費","付属金物共",1,"式"]
[null,"WD-1"]
[null,"鍵撤去／新設（引戸錠）",null,8,"か所"]
[null,"WD-1"]
[null,"鍵撤去／新設（カマ錠）",null,4,"か所"]
[null,"WD-6"]
[null,"鍵撤去／新設（引戸錠）",null,1,"か所"]
[null,"WD-7"]
[null,"鍵撤去／新設（引戸錠）",null,2,"か所"]
[null,"WD-8"]
[null,"鍵撤去／新設（引戸錠）",null,1,"か所"]
[null,"WD-9"]
[null,"鍵撤去／新設（シリンダー錠）",null,1,"か所"]
[null,"WD-10"]
[null,"鍵撤去／新設（シリンダー錠）",null,1,"か所"]
[null,"WD-13"]
[null,"鍵撤去／新設（シリンダー錠）",null,1,"か所"]
[null,"WD-14"]
[null,"鍵撤去／新設（引戸錠）",null,1,"か所"]
[null,"WD-17"]
[null,"鍵撤去／新設（シリンダー錠）",null,1,"か所"]
[null,"WD-18"]
[null,"鍵撤去／新設（シリンダー錠）",null,1,"か所"]
[null,"WD-19"]
[null,"鍵撤去／新設（引戸錠）",null,1,"か所"]
[]
[null,"サッシクリーニング",null,688,"m2"]
[]
[null,"建具廻りシーリング","MS-2　15×10程度",585,"ｍ"]
[]
[null,"建具廻りシーリング打替え","MS-2　15×10程度",712,"ｍ"]
[]
[null,"網入り型板ガラス","FWG t6.8  0.3～2.0m2",20.7,"m2"]
[]
[null,"強化ガラス","T t6 0.3～2m2",177,"m2"]
[]
[null,"強化ガラス","T t8 0.3～2m2",1.8,"m2"]
[]
[null,"型板ガラス","F t4 ～2.18m2",5.5,"m2"]
[]
[null,"ガラスクリーニング",null,1635,"m2"]
[]
[null,"ガラスシーリング","両面2倍済み",221,"ｍ"]
[null,"AW2'","t1.5"]
[null,"欄間アルミパネル撤去の上新設","W850×H300",1,"か所"]
[null,"AW8","t1.5"]
[null,"欄間アルミパネル撤去の上新設","W800×H500､W850×H500",2,"か所"]
[]
[]
[null,"SD-2"]
[null,"防火戸(床緩衝部研磨調整）","2000×2000",2,"か所"]
[null,"給食配膳室"]
[null,"握り玉撤去／新設","（シリンダー錠・サムターン）",1,"か所"]
[]
[null,"a-4　計"]
[]
[]
["a"]
[5,"(校舎)内装改修工事"]
[]
[null,"（ 撤 去 ）"]
[null,"床"]
[null,"コンクリートカッター切",null,62.8,"ｍ"]
[null,"床"]
[null,"土間コンクリート撤去",null,3.5,"m3"]
[null,"床"]
[null,"スラブコンクリート撤去",null,0.4,"m3"]
[null,"理科室床"]
[null,"断熱材撤去","t30",2.2000000000000002,"m2"]
[]
[]
[null,"床"]
[null,"モルタルカッター切",null,13.4,"ｍ"]
[null,"床"]
[null,"モルタル金鏝押え撤去",null,6.7,"m2"]
[null,"床"]
[null,"モザイクパーケット撤去",null,194,"m2"]
[null,"床"]
[null,"転ばし床撤去",null,5.4,"m2"]
[null,"床"]
[null,"コンパネ撤去","t12",5.4,"m2"]
[null,"床"]
[null,"畳撤去",null,4.5,"m2"]
[null,"床"]
[null,"カーペット撤去",null,107,"m2"]
[null,"床"]
[null,"塗床材撤去",null,577,"m2"]
[]
[]
[null,"巾木"]
[null,"雑巾摺撤去",null,8.8000000000000007,"ｍ"]
[null,"壁"]
[null,"コンクリートカッター切",null,26.8,"ｍ"]
[null,"壁"]
[null,"コンクリート撤去",null,1.4,"m3"]
[null,"壁"]
[null,"コンクリートブロック撤去",null,2.6,"m3"]
[null,"壁"]
[null,"モルタル金鏝押え撤去",null,27.8,"m2"]
[null,"壁"]
[null,"タイル撤去",null,162,"m2"]
[null,"壁"]
[null,"木間仕切り撤去",null,11,"m2"]
[null,"壁"]
[null,"石膏ボード撤去","t9",6.3,"m2"]
[null,"壁"]
[null,"耐水ベニヤ撤去",null,4.7,"m2"]
[null,"壁"]
[null,"クロス撤去",null,4.7,"m2"]
[]
[]
[null,"天井"]
[null,"軽量鉄骨天井下地撤去",null,14.3,"m2"]
[null,"天井"]
[null,"石膏ボード撤去","t9",66.400000000000006,"m2"]
[null,"天井"]
[null,"耐水石膏ボード撤去","t9.5",1.4,"m2"]
[null,"天井"]
[null,"大平板撤去","t5",84.9,"m2"]
[null,"天井"]
[null,"耐水ベニヤ撤去","t5.5",6.3,"m2"]
[null,"天井"]
[null,"クロス撤去",null,7.7,"m2"]
[]
[]
[null,"1F昇降口"]
[null,"木製モザイク掲示板撤去","W2060×H1260×D50",1,"か所"]
[null,"1F理科室"]
[null,"生徒用実験台撤去","W3010×D900×H700",3,"か所"]
[null,"1F理科室"]
[null,"映写用幕撤去","W4500×H1500",1,"か所"]
[null,"1F理科室"]
[null,"映写用幕巻上げ式ｽｸﾘｰﾝﾎﾞｯｸｽ撤去","W4500×D200",1,"か所"]
[null,"1F理科室"]
[null,"ＯＨＰスクリーン撤去","W1200×H1200",1,"か所"]
[null,"1F理科室"]
[null,"滑車吊金具撤去",null,1,"か所"]
[null,"1F給食室"]
[null,"シロッコファン用フード撤去","W4830×D1700×H1100",1,"か所"]
[null,"1F給食室"]
[null,"シロッコファン用フード撤去","W1800×D1200×H1100",1,"か所"]
[null,"1F給食室前廊下"]
[null,"下駄箱撤去","W800×D500×H750",1,"か所"]
[null,"1F給食婦室"]
[null,"押入れ撤去","W800×D900×H2300",1,"か所"]
[null,"2F職員室"]
[null,"上下黒板撤去","W2700×H1800",1,"か所"]
[null,"便所"]
[null,"ピクトサイン撤去",null,6,"か所"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"（ 改 修 ）"]
[]
[null,"内壁改修",null,1,"式"]
[]
[]
[null,"昇降口壁"]
[null,"シーリング擦り込み処理","PU-2",2.1,"ｍ"]
[]
[]
[null,"ｽﾛｰﾌﾟ床"]
[null,"１５０角タイル",null,0.7,"m2"]
[null,"ｽﾛｰﾌﾟ床"]
[null,"スロープ１５０角タイル","150角 識別しやすい色",1.2,"m2"]
[null,"便所床"]
[null,"汚垂石",null,7,"m2"]
[null,"1～3廊下壁"]
[null,"１００角タイル",null,3.3,"m2"]
[]
[]
[null,"玄関天井"]
[null,"木見切り","塗装下地",3.7,"ｍ"]
[]
[]
[null,"間仕切り"]
[null,"軽量鉄骨壁下地","W65 @300",26.2,"m2"]
[null,"間仕切り"]
[null,"軽量鉄骨壁下地","W100 @300",65.599999999999994,"m2"]
[null,"天井"]
[null,"ＬＧＳ下地 @300",null,15.5,"m2"]
[]
[null,"軽量鉄骨開口補強",null,1,"式"]
[]
[null,"天井点検口","450角",17,"か所"]
[null,"便所"]
[null,"ライニング面台","SUS HL t1.5 D1130",8.1,"ｍ"]
[null,"床"]
[null,"床見切り","SUS 40×20",2.2000000000000002,"ｍ"]
[]
[]
[null,"床"]
[null,"床見切り","SUS 40×20／120×2.0",8.5,"ｍ"]
[null,"ｽﾛｰﾌﾟ"]
[null,"手摺","SUS 2段 H550 既製品　両側共",1,"式"]
[null,"床"]
[null,"モルタル金鏝押え","貼物下地",73.599999999999994,"m2"]
[null,"床"]
[null,"モルタル塗り","ﾀｲﾙ下地",7,"m2"]
[null,"ｽﾛｰﾌﾟ床"]
[null,"モルタル塗り","ﾀｲﾙ下地",0.7,"m2"]
[null,"ｽﾛｰﾌﾟ床"]
[null,"スロープモルタル塗り","ﾀｲﾙ下地",1.2,"m2"]
[null,"ｽﾛｰﾌﾟ立上り"]
[null,"打放し補修","吹付下地",2.7,"m2"]
[null,"ｽﾛｰﾌﾟ立上り天端"]
[null,"コンクリート金鏝押え","W150 吹付下地",3.6,"ｍ"]
[null,"ｽﾛｰﾌﾟ立上り"]
[null,"複層塗材Ｅ","RC面 天端含む",3.2,"m2"]
[null,"ﾎﾟﾝﾌﾟ基礎天端"]
[null,"コンクリート金鏝押え","仕上げ",0.4,"m2"]
[null,"ﾎﾟﾝﾌﾟ基礎側面"]
[null,"打放し補修","仕上げ",1,"m2"]
[null,"壁"]
[null,"モルタル塗り","ﾀｲﾙ下地",3.3,"m2"]
[null,"壁"]
[null,"モルタル金鏝押え","t20 吹付下地",1.8,"m2"]
[null,"西階段壁"]
[null,"下地調整材","C-2",211,"m2"]
[null,"西階段､玄関壁"]
[null,"多彩模様吹付","既存ﾓﾙﾀﾙ面 ",364,"m2"]
[null,"給食室壁"]
[null,"ペーパー掛け",null,72.599999999999994,"m2"]
[null,"給食室､ｶｳﾝｾﾘﾝｸﾞﾙｰﾑ壁"]
[null,"複層塗材Ｅ","既存ﾓﾙﾀﾙ面 下地調整",100,"m2"]
[null,"給食室壁"]
[null,"複層塗材Ｅ","ﾓﾙﾀﾙ面",1.8,"m2"]
[null,"ｶｳﾝｾﾘﾝｸﾞﾙｰﾑ壁"]
[null,"複層塗材Ｅ","ﾎﾞｰﾄﾞ面",1.8,"m2"]
[]
[]
[null,"1F床"]
[null,"弾性ウレタン塗床","t2 平滑仕上げ ﾉﾝｽﾘｯﾌﾟ",178,"m2"]
[null,"2～3F床"]
[null,"弾性ウレタン塗床","t2 平滑仕上げ ﾉﾝｽﾘｯﾌﾟ",190,"m2"]
[null,"床"]
[null,"ライン","黄色",157,"ｍ"]
[null,"1F階段"]
[null,"弾性ウレタン塗床","t2 平滑仕上げ ﾉﾝｽﾘｯﾌﾟ",79.3,"m2"]
[null,"2～3F階段"]
[null,"弾性ウレタン塗床","t2 平滑仕上げ ﾉﾝｽﾘｯﾌﾟ",130,"m2"]
[null,"階段"]
[null,"ライン","黄色",107,"ｍ"]
[null,"床"]
[null,"モザイクパーケット",null,194,"m2"]
[null,"床"]
[null,"長尺塩ビシート","t2",14.6,"m2"]
[null,"床"]
[null,"長尺塩ビシート","t2.5",59,"m2"]
[null,"床"]
[null,"カーペットタイル","t6.5",107,"m2"]
[null,"巾木"]
[null,"ソフト","H75",107,"ｍ"]
[null,"壁"]
[null,"石膏ボード","t12.5 GL工法",143,"m2"]
[null,"壁"]
[null,"石膏ボード","t12.5 LGS面",124,"m2"]
[null,"天井"]
[null,"石膏ボード","t9.5 LGS面",14.6,"m2"]
[null,"壁"]
[null,"耐水石膏ボード","t12.5 GL工法",9,"m2"]
[null,"壁"]
[null,"耐水石膏ボード","t12.5 LGS面",12.3,"m2"]
[null,"壁"]
[null,"化粧珪酸カルシウム板","t6",262,"m2"]
[null,"壁"]
[null,"耐水合板","t12",10.5,"m2"]
[null,"壁化粧ｹｲｶﾙ目地"]
[null,"シーリング","SR-1 5×5",524,"ｍ"]
[]
[]
[null,"天井"]
[null,"珪酸カルシウム板","t6 LGS面",145,"m2"]
[null,"天井"]
[null,"ロックウール吸音板","t9 LGS面 PBt9.5共",106,"m2"]
[null,"ｶｳﾝｾﾘﾝｸﾞﾙｰﾑ､便所壁"]
[null,"クロス","ﾎﾞｰﾄﾞ面",22.7,"m2"]
[null,"ｶｳﾝｾﾘﾝｸﾞﾙｰﾑ､便所天井"]
[null,"クロス","ﾎﾞｰﾄﾞ面",14.6,"m2"]
[null,"廻り縁"]
[null,"塩ビ",null,204,"ｍ"]
[null,"間仕切り内"]
[null,"グラスウール充填","t100",57,"m2"]
[null,"ｶｳﾝｾﾘﾝｸﾞﾙｰﾑ壁"]
[null,"発泡ウレタン吹付","t20",22.7,"m2"]
[]
[null,"石膏ﾎﾞｰﾄﾞ継目処理",null,37.299999999999997,"m2"]
[null,"1.2F廊下"]
[null,"ステンレス手洗いＡ","W5520×D480×H500",2,"か所"]
[null,"3F廊下"]
[null,"ステンレス手洗いＡ","W4760×D480×H500",1,"か所"]
[null,"1～3F廊下"]
[null,"ステンレス手洗いＢ","W1740×D480×H500",3,"か所"]
[]
[]
[null,"1F理科室"]
[null,"生徒用調理台","W3200×D900×H750",3,"か所"]
[]
[]
[null,"1F校長室"]
[null,"耐火ロッカー一時撤去再設置","W1050×D650×H1050",1,"か所"]
[]
[]
[null,"便所"]
[null,"ピクトサイン","平付　300×300　ｱｸﾘﾙ板　ｶｯﾃｨﾝｸﾞｼｰﾄ貼り",5,"か所"]
[null,"便所"]
[null,"ピクトサイン","持出し　　300×300　ｱｸﾘﾙ板　ｶｯﾃｨﾝｸﾞｼｰﾄ貼り",2,"か所"]
[null,"1F昇降口"]
[null,"掲示板","W2000×H1200",1,"か所"]
[]
[]
[null,"2F職員室"]
[null,"上下ホワイトボード","W2700×H1800",1,"か所"]
[]
[]
[]
[]
[]
[null,"a-5　計"]
[]
[]
["a"]
[6,"(校舎)塗装改修工事"]
[null,"（ 外 部 ）屋根平場ﾀﾗｯﾌﾟ"]
[null,"ＤＰ塗り替え","下地処理共",14.2,"ｍ"]
[null,"ﾍﾞﾗﾝﾀﾞ手摺"]
[null,"ＤＰ塗り替え","下地処理共",307,"ｍ"]
[null,"竪樋養生管"]
[null,"ＤＰ塗り替え","下地処理共",36,"ｍ"]
[null,"竪樋","100φ"]
[null,"ＤＰ塗り替え","下地処理共",156,"ｍ"]
[null,"（ 内 部 ）ｶｳﾝｾﾘﾝｸﾞﾙｰﾑ壁"]
[null,"ＥＰ-Ｇ","ﾎﾞｰﾄﾞ面",1.8,"m2"]
[null,"便所天井"]
[null,"ＥＰ－Ｇ","ｹｲｶﾙ面",145,"m2"]
[null,"便所天井"]
[null,"ＥＰ－Ｇ","既存ﾓﾙﾀﾙ面 下地処理共",3.1,"m2"]
[null,"玄関天井"]
[null,"ＳＯＰ","木部細物",3.7,"ｍ"]
[null,"木製建具"]
[null,"ＳＯＰ","木部",23.6,"m2"]
[null,"3F廊下壁"]
[null,"ＳＯＰ塗り替え","描画面 RA種下地調整共",9.3000000000000007,"m2"]
[null,"3F廊下木製建具"]
[null,"ＳＯＰ塗り替え","描画面 RA種下地調整共",9,"m2"]
[null,"掲示板枠"]
[null,"ＳＯＰ塗り替え","木部細物 下地調整共",6.6,"ｍ"]
[null,"壁見切り"]
[null,"ＳＯＰ塗り替え","木部細物 下地調整共",2.6,"ｍ"]
[]
[]
[]
[null,"a-6　計"]
[]
[]
["a"]
[7,"(校舎)躯体改修工事"]
[]
[null,"（ 外 部 ）","ｽﾛｰﾌﾟ"]
[]
[null,"鋤取り",null,1,"m3"]
[]
[null,"残土処分",null,1,"m3"]
[]
[null,"砕石地業",null,1,"m3"]
[]
[null,"異形鉄筋","SD295A D10",0.1,"ｔ"]
[]
[null,"異形鉄筋","SD295A D13",0.1,"ｔ"]
[]
[null,"鉄筋加工組立費",null,0.2,"ｔ"]
[]
[null,"鉄筋運搬費",null,0.2,"ｔ"]
[]
[]
[]
[null,"差し筋アンカー","D10 横向き",11,"か所"]
[null,"土間"]
[null,"普通コンクリート",null,3.3,"m3"]
[null,"土間"]
[null,"コンクリート打設費",null,3.3,"m3"]
[]
[null,"コンクリートポンプ車","基本料",1,"台"]
[]
[]
[]
[null,"普通型枠",null,1.9,"m2"]
[]
[null,"型枠運搬費",null,9.6,"m2"]
[]
[null,"打放し型枠",null,7.7,"m2"]
[]
[]
[]
[null,"（ 内 部 ）","床､ｽﾛｰﾌﾟ､便器撤去跡､ﾎﾟﾝﾌﾟ基礎"]
[]
[null,"砕石地業","土間下",2.2000000000000002,"m3"]
[null,"床"]
[null,"ポリエチレンシート","t0.15",24.3,"m2"]
[null,"理科室床"]
[null,"スタイロフォーム","t30",2.2000000000000002,"m2"]
[null,"便所床"]
[null,"スタイロフォーム","t50",22.1,"m2"]
[null,"便所踏込み床"]
[null,"スタイロフォーム","t75",6.6,"m2"]
[]
[null,"異形鉄筋","SD295A D10",20,"㎏"]
[]
[null,"異形鉄筋","SD295A D13",20,"㎏"]
[]
[null,"鉄筋加工組立費",null,90,"㎏"]
[]
[null,"鉄筋運搬費",null,90,"㎏"]
[]
[]
[null,"床"]
[null,"溶接金網","6φ-150　敷き手間共",30.1,"m2"]
[]
[]
[null,"床"]
[null,"差し筋アンカー","D10 横向き",400,"か所"]
[null,"土間"]
[null,"普通コンクリート",null,4.0999999999999996,"m3"]
[null,"ｽﾗﾌﾞ"]
[null,"普通コンクリート",null,0.4,"m3"]
[null,"ﾎﾟﾝﾌﾟ基礎"]
[null,"普通コンクリート",null,0.1,"m3"]
[null,"踏込み床"]
[null,"軽量コンクリート",null,0.4,"m2"]
[null,"土間"]
[null,"コンクリート打設費",null,4.0999999999999996,"m3"]
[]
[]
[null,"ｽﾗﾌﾞ"]
[null,"コンクリート打設費",null,0.4,"m3"]
[null,"ﾎﾟﾝﾌﾟ基礎"]
[null,"コンクリート打設費",null,0.1,"m3"]
[null,"踏込み床軽量ｺﾝ"]
[null,"コンクリート打設費",null,0.4,"m2"]
[null,"便器撤去跡"]
[null,"普通型枠",null,2.4,"m2"]
[null,"ｽﾛｰﾌﾟ床"]
[null,"打放し型枠",null,2.7,"m2"]
[null,"ﾎﾟﾝﾌﾟ基礎"]
[null,"打放し型枠",null,1,"m2"]
[]
[null,"型枠運搬費",null,6.1,"m2"]
[]
[null,"コンクリートポンプ車","基本料",4,"台"]
[]
[]
[]
[]
[]
[null,"a-7　計"]
[]
[]
["a"]
[8,"(校舎)環境配慮改修工事"]
[]
[null,"（ 内 部 ）"]
[null,"天井"]
[null,"ロックウール吸音板撤去","t12 ｱｽﾍﾞｽﾄ含有",106,"m2"]
[null,"天井"]
[null,"石膏ボード撤去","t9.5",106,"m2"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"a-8　計"]
[]
[]
["a"]
[9,"(校舎)発生材積込運搬費"]
[]
[null,"発生材集積積込費","ｺﾝｸﾘｰﾄ・ﾓﾙﾀﾙ類等・人力",17.5,"ｍ3"]
[]
[null,"発生材集積積込費","内装・木材等・人力",15.5,"ｍ3"]
[]
[]
[]
[null,"発生材運搬費","ｺﾝｸﾘｰﾄ・ﾓﾙﾀﾙ類等・人力",17.5,"ｍ3"]
[]
[null,"発生材運搬費","内装・木材等・人力",15.5,"ｍ3"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"a-9　計"]
[]
[]
["a"]
[10,"(校舎)発生材処分費"]
[]
[null,"発生材処分費","ｺﾝｸﾘｰﾄ・モルタル",40.200000000000003,"ｔ"]
[]
[null,"発生材処分費","砕石",2.5,"ｔ"]
[]
[null,"発生材処分費","ﾎﾞｰﾄﾞ",1.4,"ｔ"]
[]
[null,"発生材処分費","木材",2.2999999999999998,"ｔ"]
[]
[null,"発生材処分費","ﾌﾟﾗｽﾁｯｸ",1.1000000000000001,"㎥"]
[]
[null,"発生材処分費","混合廃棄物",0.8,"ｔ"]
[]
[null,"発生材処分費","ｶﾞﾗｽ",0.7,"ｔ"]
[]
[null,"発生材処分費","繊維類",132,"㎏"]
[]
[null,"発生材処分費","ｸﾛｽ",1.1000000000000001,"㎥"]
[]
[null,"発生材処分費","ｱｽﾌｧﾙﾄ防水",1.5,"ｔ"]
[]
[null,"発生材処分費","ｱｽﾍﾞｽﾄ成形板",0.4,"ｔ"]
[]
[null,"有価物控除","ｽﾁｰﾙ H2",-0.72,"ｔ"]
[]
[null,"有価物控除","ｽﾁｰﾙ H4",-3.9,"ｔ"]
[]
[null,"有価物控除","ｱﾙﾐ",-3.4,"ｔ"]
[]
[null,"a-10　計"]
[]
[]
[]
["b","屋内運動場改修工事"]
[]
[1,"(屋内運動場）直接仮設工事",null,1,"式"]
[]
[2,"(屋内運動場）外壁改修工事",null,1,"式"]
[]
[3,"(屋内運動場）建具改修工事",null,1,"式"]
[]
[4,"(屋内運動場）内装改修工事",null,1,"式"]
[]
[5,"(屋内運動場）塗装改修工事",null,1,"式"]
[]
[6,"(屋内運動場）発生材積込運搬費",null,1,"式"]
[]
[7,"(屋内運動場）発生材処分費",null,1,"式"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ｂ　計"]
[]
[]
["ｂ"]
[1,"(屋内運動場）直接仮設工事"]
[null,"（ 外 部 ）外壁改修"]
[null,"墨出し",null,187,"m2"]
[null,"外壁改修"]
[null,"養生",null,218,"m2"]
[null,"外壁改修"]
[null,"整理清掃後片付け",null,218,"m2"]
[]
[null,"くさび緊結式足場","W1200",518,"m2"]
[]
[null,"養生シート",null,798,"m2"]
[]
[null,"くさび緊結式足場","W600",280,"m2"]
[]
[null,"安全手摺",null,109,"m2"]
[]
[null,"脚立足場",null,24,"m2"]
[]
[]
[null,"（ 内 部 ）内装改修"]
[null,"墨出し",null,454,"m2"]
[null,"内装改修"]
[null,"養生",null,454,"m2"]
[null,"内装改修"]
[null,"整理清掃後片付け",null,454,"m2"]
[null,"内装改修"]
[null,"内部足場","脚立",8,"m2"]
[]
[null,"ローリングタワー","H8000",1,"か所"]
[]
[null,"ｂ-1　計"]
[]
[]
["ｂ"]
[2,"(屋内運動場）外壁改修工事"]
[]
[null,"（ 撤 去 ）"]
[null,"軒天"]
[null,"珪酸カルシウム板撤去","t6",10.8,"m2"]
[null,"ｽﾛｰﾌﾟ"]
[null,"土間コンクリートカッター切り",null,5.2,"ｍ"]
[null,"ｽﾛｰﾌﾟ"]
[null,"砕石撤去",null,0.4,"m3"]
[null,"ｽﾛｰﾌﾟ"]
[null,"土間コンクリート撤去",null,0.6,"m3"]
[]
[null,"校章撤去","1200φ　積込・運搬共",1,"か所"]
[]
[null,"館名板撤去","積込・運搬共",1,"か所"]
[]
[null,"（ 改 修 ）"]
[null,"外壁"]
[null,"外壁用塗膜防水材","ALC面",144,"m2"]
[null,"外壁"]
[null,"クラック補修","0.5㎜以上　クラック部下地挙動緩衝材共",29.8,"ｍ"]
[null,"軒天"]
[null,"珪酸カルシウム板","t6",10.8,"m2"]
[null,"軒天"]
[null,"廻縁",null,14.5,"ｍ"]
[]
[null,"校章","1200φ",1,"か所"]
[]
[null,"館名板",null,1,"か所"]
[]
[null,"（ スロープ ）"]
[]
[null,"鋤取り",null,1.4,"m3"]
[]
[null,"残土処分",null,1.4,"m3"]
[]
[null,"砕石地業","土間下",0.6,"m3"]
[]
[null,"異形鉄筋","SD295A D10",0.1,"ｔ"]
[]
[null,"異形鉄筋","SD295A D13",0.3,"ｔ"]
[]
[null,"鉄筋加工組立費",null,0.4,"ｔ"]
[]
[null,"鉄筋運搬費",null,0.4,"ｔ"]
[]
[]
[]
[null,"差し筋アンカー","D10 横向き",28,"か所"]
[null,"土間"]
[null,"普通コンクリート",null,1.7,"m3"]
[]
[null,"コンクリート打設費",null,1.7,"m3"]
[]
[null,"コンクリートポンプ車","基本料",1,"台"]
[]
[null,"普通型枠",null,1.5,"m2"]
[]
[null,"打放し型枠",null,6.1,"m2"]
[]
[null,"型枠運搬費",null,7.6,"m2"]
[null,"床"]
[null,"磁器質タイル","150角",2,"m2"]
[null,"ｽﾛｰﾌﾟ"]
[null,"磁器質タイル","150角 色分け",3.1,"m2"]
[null,"ｽﾛｰﾌﾟ"]
[null,"点状タイル",null,0.3,"m2"]
[]
[null,"手摺","SUS H550 2段　両側共",1,"式"]
[null,"床"]
[null,"モルタル塗り","ﾀｲﾙ下地",2.2999999999999998,"m2"]
[null,"ｽﾛｰﾌﾟ"]
[null,"モルタル塗り","ﾀｲﾙ下地",3.1,"m2"]
[null,"犬走り"]
[null,"モルタル金鏝押え","仕上げ",0.7,"m2"]
[null,"立上り"]
[null,"打放し補修","吹付下地",6.1,"m2"]
[null,"立上り天端"]
[null,"コンクリート金鏝押え","W150 吹付下地",10,"ｍ"]
[null,"立上り"]
[null,"複層塗材Ｅ","天端含む",7.6,"m2"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ｂ-2　計"]
[]
[]
["ｂ"]
[3,"(屋内運動場）建具改修工事"]
[]
[null,"（ 撤 去 ）"]
[]
[null,"引分けハンガードア撤去","2430×2020",1,"か所"]
[]
[]
[]
[null,"（ 新 設 ）"]
[null,"HD-2"]
[null,"片引きフラッシュハンガー戸","1040×2012　取付調整費共",1,"か所"]
[null,"HD-3"]
[null,"片引きフラッシュハンガー戸","1040×2015　取付調整費共",1,"か所"]
[]
[]
[]
[null,"（ 改 修 ）"]
[null,"(既設）HD-1","開閉調整､引戸錠取替え"]
[null,"引分けフラッシュハンガー戸","2400×2000",1,"か所"]
[]
[]
[null,null,"壁式固定式バスケットゴール"]
[null,"既存運動器具補修","フレーム塗装補修、ゴールネット補修、清掃等",4,"か所"]
[]
[]
[]
[]
[]
[]
[]
[null,"ｂ-3　計"]
[]
[]
["ｂ"]
[4,"(屋内運動場）内装改修工事"]
[]
[null,"（ 撤 去 ）"]
[null,"床"]
[null,"既設塗床目荒し",null,446,"㎡"]
[null,"巾木"]
[null,"木製巾木撤去","H100",9,"ｍ"]
[null,"壁"]
[null,"木間仕切り撤去",null,3.6,"m2"]
[null,"壁"]
[null,"胴縁撤去",null,29,"m2"]
[null,"壁"]
[null,"シナベニヤ撤去","t9",2.5,"m2"]
[null,"壁"]
[null,"シナベニヤ撤去","t5.5",26.5,"m2"]
[null,"天井"]
[null,"木野縁撤去",null,8,"m2"]
[null,"天井"]
[null,"ラワンベニヤ撤去","t5.5",8,"m2"]
[]
[]
[null,"体育用具室A"]
[null,"ポスト台撤去","支柱共",1,"か所"]
[null,"ｽﾃｰｼﾞ上部　"]
[null,"校章撤去",null,1,"か所"]
[]
[null,"演台校章撤去",null,1,"か所"]
[]
[null,"（ 改 修 ）"]
[null,"間仕切り"]
[null,"木間仕切り下地",null,20.100000000000001,"m2"]
[null,"壁"]
[null,"胴縁",null,38.1,"m2"]
[null,"巾木"]
[null,"木製巾木","米栂 H100",4.9000000000000004,"ｍ"]
[null,"壁"]
[null,"シナ有孔ベニヤ","t9 目透し",3.2,"m2"]
[null,"壁"]
[null,"ラワンベニヤ","t5.5 目透し",13,"m2"]
[null,"天井"]
[null,"木野縁",null,8,"m2"]
[]
[]
[]
[null,"天井点検口","ｱﾙﾐ製 450角",2,"か所"]
[]
[null,"軽量鉄骨天井下地開口補強","450角",2,"か所"]
[null,"多目的便所"]
[null,"ライニング面台","SUS HL t1.5 D130",6.2,"ｍ"]
[null,"床"]
[null,"屋内スポーツ用長尺弾性塩ビシート","t7.5　既設塗床目荒し共",446,"m2"]
[null,"床"]
[null,"端部処理ｼｰﾘﾝｸﾞ","ｼｰﾄ外周",25.2,"ｍ"]
[null,"床"]
[null,"防滑性長尺塩ビシート","t2.5",8,"m2"]
[null,"巾木"]
[null,"ソフト","H300",10.3,"ｍ"]
[null,"壁"]
[null,"石膏ボード","t12.5 LGS面",21.9,"m2"]
[null,"壁"]
[null,"耐水石膏ボード","t12.5 LGS面",3.1,"m2"]
[null,"壁"]
[null,"耐水合板","t12",3.1,"m2"]
[null,"壁"]
[null,"化粧珪酸カルシウム板","t6",25,"m2"]
[]
[]
[null,"壁化粧ｹｲｶﾙ目地"]
[null,"シーリング","SR-1 5×5",49.9,"ｍ"]
[null,"天井"]
[null,"珪酸カルシウム板","t6",8,"m2"]
[]
[null,"廻縁","塩ﾋﾞ",19.399999999999999,"ｍ"]
[]
[]
[null,"体育館"]
[null,"暗幕","W1450×H1200　撤去費共",2,"か所"]
[null,"体育館"]
[null,"暗幕","W5050×H3300　撤去費共",10,"か所"]
[null,"体育館"]
[null,"暗幕","W4500×H2600　撤去費共",1,"か所"]
[]
[null,"以上暗幕取付調整費",null,1,"式"]
[]
[null,"塩ﾋﾞｼｰﾄ押えへの字金物　","L800",4,"本"]
[]
[null,"塩ﾋﾞｼｰﾄ押えへの字金物　","L1000",2,"本"]
[]
[null,"塩ﾋﾞｼｰﾄ押えへの字金物　","L11000",1,"本"]
[]
[null,"塩ﾋﾞｼｰﾄ押えへの字金物　","L2700",2,"本"]
[]
[null,"塩ﾋﾞｼｰﾄ押えへの字金物　","L1800",2,"本"]
[]
[null,"ステージ上校章",null,1,"か所"]
[]
[null,"演台　校章",null,1,"か所"]
[]
[]
[null,"既設ﾊﾞﾚｰﾎﾞｰﾙ"]
[null,"床金具撤去","充填ﾓﾙﾀﾙ共",2,"か所"]
[null,"既設ﾊﾞﾄﾞﾐﾝﾄﾝ"]
[null,"床金具撤去","充填ﾓﾙﾀﾙ共",2,"か所"]
[null,"新設ﾊﾞﾚｰﾎﾞｰﾙ"]
[null,"床金具","埋設管共　材工共",2,"か所"]
[null,"新設ﾊﾞﾄﾞﾐﾝﾄﾝ"]
[null,"床金具","埋設管共　材工共",2,"か所"]
[]
[]
[null,"体育館"]
[null,"バレーボールコート（６人制）","18000×9000",1,"面"]
[null,"体育館"]
[null,"バトミントンコート","13400×6000",1,"面"]
[null,"体育館"]
[null,"ポートボールコート","14000×9000",2,"面"]
[]
[]
[]
[null,"床洗浄",null,446,"㎡"]
[]
[]
[]
[null,"金属製防球カバー",null,1,"か所"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ｂ-4　計"]
[]
[]
["ｂ"]
[5,"(屋内運動場）塗装改修工事"]
[]
[null,"（ 外 部 ）"]
[null,"軒天"]
[null,"ＥＰ-Ｇ","ｹｲｶﾙ面",10.8,"m2"]
[null,"軒天"]
[null,"ＥＰ-Ｇ塗り替え","ｹｲｶﾙ面 下地調整共",176,"m2"]
[]
[]
[]
[null,"（ 内 部 ）"]
[null,"壁"]
[null,"ＳＯＰ","木部",16.2,"m2"]
[null,"天井"]
[null,"ＥＰ-G","ｹｲｶﾙ面",8,"m2"]
[null,"巾木"]
[null,"ＳＯＰ","木部 H100",4.9000000000000004,"ｍ"]
[null,"多目的便所ｻｯｼ額縁"]
[null,"ＳＯＰ塗り替え","木部細物 下地調整共",6.8,"ｍ"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ｂ-5　計"]
[]
[]
["ｂ"]
[6,"(屋内運動場）発生材積込運搬費"]
[]
[null,"発生材集積積込費","ｺﾝｸﾘｰﾄ・ﾓﾙﾀﾙ類等・人力",1,"ｍ3"]
[]
[null,"発生材集積積込費","内装・木材等・人力",1.6,"ｍ3"]
[]
[]
[]
[null,"発生材運搬費","ｺﾝｸﾘｰﾄ・ﾓﾙﾀﾙ類等・人力",1,"ｍ3"]
[]
[null,"発生材運搬費","内装・木材等・人力",1.6,"ｍ3"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ｂ-6　計"]
[]
[]
["ｂ"]
[7,"(屋内運動場）発生材処分費"]
[]
[null,"発生材処分費","ｺﾝｸﾘｰﾄ・モルタル",1.5,"ｔ"]
[]
[null,"発生材処分費","砕石",1,"ｔ"]
[]
[null,"発生材処分費","ﾎﾞｰﾄﾞ",0.04,"ｔ"]
[]
[null,"発生材処分費","木材",0.3,"ｔ"]
[]
[null,"発生材処分費","繊維類",108,"㎏"]
[]
[null,"有価物控除","ｽﾁｰﾙ H2",-7.0000000000000007E-2,"ｔ"]
[]
[null,"有価物控除","ｽﾁｰﾙ H4",-0.2,"ｔ"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ｂ-7　計"]
[]
[]
[]
["ｃ","外構工事"]
[]
[1,"(外構)舗装工事",null,1,"式"]
[]
[2,"(外構)門扉１工事",null,1,"式"]
[]
[3,"(外構)門扉２工事",null,1,"式"]
[]
[4,"(外構)駐車場工事",null,1,"式"]
[]
[5,"(外構)その他工事",null,1,"式"]
[]
[6,"(外構)発生材積込運搬費",null,1,"式"]
[]
[7,"(外構)発生材処分費",null,1,"式"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ｃ　計"]
[]
[]
["ｃ"]
[1,"(外構)舗装工事"]
[]
[null,"（ 撤 去 ）"]
[null,"設備関連"]
[null,"アスファルトカッター切り",null,36.200000000000003,"ｍ"]
[null,"設備関連"]
[null,"アスファルト舗装撤去","密粒度ｱｽｺﾝt50+粒調砕石t150",15.4,"m2"]
[null,"設備関連"]
[null,"コンクリート舗装カッター切り",null,74.5,"ｍ"]
[null,"設備関連","土間ｺﾝt150+鉄筋D10@200"]
[null,"コンクリート舗装撤去","+砕石t100",10.3,"m2"]
[]
[]
[]
[null,"（ 改 修 ）"]
[null,"敷地南西"]
[null,"鋤取り",null,30.5,"m3"]
[null,"敷地南西"]
[null,"残土処分","自由処分",30.5,"m3"]
[null,"敷地南西"]
[null,"アスファルト舗装","密粒度ｱｽｺﾝt13+粒調砕石t20＋地盤改良t300",203,"m2"]
[]
[null,"地先境界ブロック","100×155　材工共",35,"ｍ"]
[null,"設備関連"]
[null,"アスファルト舗装","密粒度ｱｽｺﾝt50+粒調砕石t150",15.4,"m2"]
[null,"設備関連","土間ｺﾝt150+鉄筋D10@200"]
[null,"土間コンクリート舗装","+砕石t100",10.3,"m2"]
[]
[]
[]
[null,"ｃ-1　計"]
[]
[]
["ｃ"]
[2,"(外構)門扉１工事"]
[]
[null,"（ 撤 去 ）"]
[]
[null,"コンクリート舗装カッター切り",null,13.7,"ｍ"]
[null,null,"土間ｺﾝt150+鉄筋D10@200"]
[null,"コンクリート舗装撤去","+砕石t100",51.5,"m2"]
[]
[null,"校名板撤去",null,1,"か所"]
[]
[]
[]
[null,"（ 改 修 ）"]
[null,null,"土間ｺﾝt150+鉄筋D10@200"]
[null,"コンクリート舗装","+砕石t100",51.5,"m2"]
[]
[null,"校名板","SUS W900×H150,W150×H600",2,"か所"]
[]
[null,"大型伸縮門扉","W9533×H1050",1,"か所"]
[null,"既存門塀 1"]
[null,"高圧水洗浄",null,15.2,"m2"]
[null,"既存門塀"]
[null,"吹付けタイル","下地調整共",15.2,"m2"]
[]
[]
[]
[]
[]
[]
[]
[null,"ｃ-2　計"]
[]
[]
["ｃ"]
[3,"(外構)門扉２工事"]
[]
[null,"（ 撤 去 ）"]
[]
[null,"コンクリート舗装カッター切り",null,2.9,"ｍ"]
[null,"門扉2","土間ｺﾝt150+鉄筋D10@200"]
[null,"コンクリート舗装撤去","+砕石t100",11,"m2"]
[null,"壁"]
[null,"コンクリートカッター切り",null,1,"ｍ"]
[]
[null,"基礎コンクリート撤去",null,0.7,"m3"]
[]
[null,"撤去跡埋戻し",null,0.2,"m3"]
[null,"桜大"]
[null,"枝剪定","H4000程度",1,"か所"]
[null,"桜中"]
[null,"枝剪定","H2000程度",1,"か所"]
[]
[null,"（ 改 修 ）"]
[]
[null,"鋤取り",null,8.5,"m3"]
[]
[null,"根切",null,3.1,"m3"]
[]
[null,"埋戻し",null,2.4,"m3"]
[]
[null,"残土処分","自由処分",9.1999999999999993,"m3"]
[]
[null,"床付け",null,2,"m2"]
[]
[null,"砕石地業","基礎下",0.2,"m3"]
[]
[null,"異形鉄筋","SD295A D10",0.04,"ｔ"]
[]
[null,"異形鉄筋","SD295A D13",0.02,"ｔ"]
[]
[null,"鉄筋加工組立費",null,0.05,"ｔ"]
[]
[null,"鉄筋運搬費",null,0.05,"ｔ"]
[]
[]
[null,"捨て"]
[null,"普通コンクリート",null,0.1,"m3"]
[null,"基礎"]
[null,"普通コンクリート",null,0.9,"m3"]
[null,"捨て"]
[null,"コンクリート打設費",null,0.1,"m3"]
[null,"基礎"]
[null,"コンクリート打設費",null,0.9,"m3"]
[]
[null,"コンクリートポンプ車","基本料",2,"台"]
[]
[]
[]
[]
[]
[null,"基礎型枠",null,2.9,"m2"]
[]
[null,"打放し型枠",null,6.5,"m2"]
[]
[null,"型枠運搬費",null,9.4,"m2"]
[null,"立上り"]
[null,"打放し補修","吹付下地",6.5,"m2"]
[null,"立上り天端"]
[null,"コンクリート金鏝押え","吹付下地",0.5,"m2"]
[null,"立上り"]
[null,"吹付けタイル","天端含む",7,"m2"]
[null,null,"土間ｺﾝt150+鉄筋D10@200"]
[null,"コンクリート舗装","+砕石t100",32.1,"m2"]
[]
[null,"スチールグレーチング 嵩上げ","W300嵩上タイプ　車道用　騒音防止タイプ　Ｔ-20",2,"ｍ"]
[]
[null,"大型伸縮門扉","W5245×H1050",1,"か所"]
[null,"既設Ｕ字溝蓋"]
[null,"スチールグレーチング新設","Ｕ-300用　車道用　騒音防止タイプ　Ｔ-20",9,"ｍ"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ｃ-3　計"]
[]
[]
["ｃ"]
[4,"(外構)駐車場工事"]
[]
[null,"（ 撤 去 ）"]
[]
[null,"コンクリート舗装カッター切り",null,11.5,"ｍ"]
[]
[null,"コンクリート舗装撤去",null,32.799999999999997,"m2"]
[]
[null,"コンクリート蓋撤去","W240",10.3,"ｍ"]
[]
[null,"Ｕ字溝撤去",null,10.3,"ｍ"]
[]
[null,"（ 改 修 ）"]
[]
[null,"鋤取り",null,27,"m3"]
[]
[null,"残土処分","自由処分　",27,"m3"]
[null,null,"土間ｺﾝt150+鉄筋D10@200"]
[null,"コンクリート舗装","+砕石t100",146,"m2"]
[]
[null,"車止めブロック","歩車道境界ブロックＡ",4,"か所"]
[]
[null,"ライン引き",null,24,"ｍ"]
[]
[null,"ゼブラゾーン","5000×1200",2,"か所"]
[]
[null,"身障者シンボルマーク",null,2,"か所"]
[]
[null,"既設桝蓋嵩上げ","600角",1,"か所"]
[]
[null,"既設桝蓋嵩上げ","500角",1,"か所"]
[]
[null,"既設桝蓋嵩上げ","300φ",1,"か所"]
[]
[null,"既設桝蓋嵩上げ","200φ",2,"か所"]
[]
[null,"既設桝蓋嵩上げ","100φ",4,"か所"]
[]
[null,"バリカー横型","Ｌ2000　基礎共",4,"か所"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ｃ-4　計"]
[]
[]
["ｃ"]
[5,"(外構)その他工事"]
[null,"1石造"]
[null,"基礎コンクリート撤去",null,1.2,"m3"]
[null,"1石造"]
[null,"埋戻し",null,0.3,"m3"]
[null,"2花壇"]
[null,"基礎コンクリート撤去",null,2.2999999999999998,"m3"]
[null,"2花壇"]
[null,"埋戻し",null,0.6,"m3"]
[null,"3鳥小屋"]
[null,"基礎砕石撤去",null,0.2,"m3"]
[null,"3鳥小屋"]
[null,"基礎コンクリート撤去",null,0.5,"m3"]
[null,"3鳥小屋"]
[null,"Ｓ造上屋撤去",null,1.6,"m2"]
[null,"3鳥小屋"]
[null,"埋戻し",null,0.5,"m3"]
[null,"4うさぎ小屋"]
[null,"基礎砕石撤去",null,1.8,"m3"]
[null,"4うさぎ小屋"]
[null,"基礎コンクリート撤去",null,4.9000000000000004,"m3"]
[null,"4うさぎ小屋"]
[null,"木造上屋撤去",null,15.2,"m2"]
[null,"4うさぎ小屋"]
[null,"埋戻し",null,2.6,"m3"]
[null,"5池"]
[null,"基礎砕石撤去",null,1.5,"m3"]
[null,"5池"]
[null,"基礎コンクリート撤去",null,3.9,"m3"]
[null,"5池"]
[null,"埋戻し",null,10.7,"m3"]
[]
[]
[null,"6足洗い場"]
[null,"基礎砕石撤去",null,0.3,"m3"]
[null,"6足洗い場"]
[null,"基礎コンクリート撤去",null,1,"m3"]
[null,"6足洗い場"]
[null,"埋戻し",null,0.6,"m3"]
[null,"7花壇"]
[null,"基礎砕石撤去",null,1.2,"m3"]
[null,"7花壇"]
[null,"基礎コンクリート撤去",null,3.7,"m3"]
[null,"7花壇"]
[null,"小低木撤去","1000φ H1200",11,"か所"]
[null,"7花壇"]
[null,"埋戻し",null,2.5,"m3"]
[null,"10卒業制作1"]
[null,"基礎砕石撤去",null,0.3,"m3"]
[null,"10卒業制作1"]
[null,"基礎コンクリート撤去",null,0.7,"m3"]
[null,"10卒業制作1"]
[null,"埋戻し",null,0.1,"m3"]
[]
[]
[null,"12卒業制作2"]
[null,"基礎砕石撤去",null,0.1,"m3"]
[null,"12卒業制作2"]
[null,"基礎コンクリート撤去",null,0.7,"m3"]
[null,"12卒業制作2"]
[null,"埋戻し",null,0.2,"m3"]
[null,"13ﾄｰﾃﾑﾎﾟｰﾙ"]
[null,"トーテムポール撤去","200φ H3700",5,"か所"]
[null,"13ﾄｰﾃﾑﾎﾟｰﾙ"]
[null,"埋戻し",null,0.1,"m3"]
[]
[]
[null,"14校名板撤去"]
[null,"校名板撤去","SUS W900×H150",1,"か所"]
[null,"15得点板"]
[null,"基礎コンクリート撤去",null,0.1,"m3"]
[null,"15得点板"]
[null,"得点板撤去","W1900×H1800",1,"か所"]
[null,"15得点板"]
[null,"埋戻し",null,0.1,"m3"]
[null,"16脱輪防止柵"]
[null,"脱輪防止柵撤去","W1100×H350",1,"ヶ所"]
[null,"17正門"]
[null,"ＤＰ塗り替え","下地処理共",15.4,"㎡"]
[null,"17正門"]
[null,"錠前取付金具調整","下地処理共",1,"か所"]
[null,"18ｶﾞｰﾄﾞﾊﾟｲﾌﾟ"]
[null,"基礎砕石撤去",null,0.2,"m3"]
[null,"18ｶﾞｰﾄﾞﾊﾟｲﾌﾟ"]
[null,"基礎コンクリート撤去",null,0.2,"m3"]
[null,"18ｶﾞｰﾄﾞﾊﾟｲﾌﾟ"]
[null,"ガードパイプ撤去","W3000×H800",3,"か所"]
[null,"18ｶﾞｰﾄﾞﾊﾟｲﾌﾟ"]
[null,"埋戻し",null,0.3,"m3"]
[null,"19ﾀｲﾔ遊具"]
[null,"タイヤ遊具撤去","1400φ×D400",3,"か所"]
[null,"21百葉箱"]
[null,"百葉箱台撤去","SUS W1050×D1050×H1000",1,"か所"]
[null,"22防球ﾈｯﾄ"]
[null,"防球ネット加工","車通行口拡大　出入口加工・補修",1,"式"]
[]
[null,"ジャングルジム設置","2750×2750×Ｈ2810　基礎施工共",1,"ヶ所"]
[]
[null,"ｃ-5　計"]
[]
[]
["ｃ"]
[6,"(外構)発生材積込運搬費"]
[]
[null,"発生材集積積込費","ｺﾝｸﾘｰﾄ・ﾓﾙﾀﾙ類等・人力",74.3,"ｍ3"]
[]
[null,"発生材集積積込費","内装・木材等・人力",11.9,"ｍ3"]
[]
[]
[]
[null,"発生材運搬費","ｺﾝｸﾘｰﾄ・ﾓﾙﾀﾙ類等・人力",74.3,"ｍ3"]
[]
[null,"発生材運搬費","内装・木材等・人力",11.9,"ｍ3"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ｃ-6　計"]
[]
[]
["ｃ"]
[7,"(外構)発生材処分費"]
[]
[null,"発生材処分費","ｺﾝｸﾘｰﾄ",94.3,"ｔ"]
[]
[null,"発生材処分費","砕石",74.8,"ｔ"]
[]
[null,"発生材処分費","ｱｽﾌｧﾙﾄ",14.4,"ｔ"]
[]
[null,"発生材処分費","樹木",0.6,"ｔ"]
[]
[null,"発生材処分費","木材",0.3,"ｔ"]
[]
[null,"発生材処分費","ﾌﾟﾗｽﾁｯｸ",0.3,"㎥"]
[]
[null,"発生材処分費","混合廃棄物",2.5,"ｔ"]
[]
[null,"発生材処分費","ﾀｲﾔ",0.03,"ｔ"]
[]
[null,"有価物控除","ｽﾁｰﾙH2",-3.31,"ｔ"]
[]
[null,"有価物控除","ｽﾁｰﾙH4",-0.4,"ｔ"]
[]
[null,"有価物控除","SUS",-0.03,"ｔ"]
[]
[]
[]
[]
[]
[]
[]
[null,"ｃ-7　計"]
[]
[]
[]
["B","共通仮設工事","積上げ分"]
[]
[null,"仮囲い","H1800",80,"ｍ"]
[]
[null,"クロスゲート","W5000×H1800",1,"か所"]
[]
[null,"交通誘導員","1人／日",100,"人"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Ｂ　計"]